[  233.216865] [hdmitx:] pll_od0 = 1, pll_od2 = 1, pll_od1 = 2
[  233.217253] [hdmitx:] clocks_set_vid_clk_div_for_hdmi[402] div = 6
[  233.218182] [hdmitx:] configure venc
[  233.218741] [hdmitx:] config_tv_enc_calc[63] vic = 95
[  233.219520] [hdmitx:] hdmitx_soft_reset[1263]
[  233.220209] [hdmitx:]  config hdmitx IP vic = 95 cd:6 cs: 1
[  233.221057] [hdmitx:] configure hdmitx21
[  233.221671] [hdmitx:] warn: SCDC not present, should not send 1:10
[  233.223633] [hdmitx:] enable phy to dig
[  233.223693] [hdmitx:] hdmitx_set_dispmode[1551] frl_rate 0 htotal 4400 cs 1 cd 6 h_unstable 0
[  233.264640] [hdmitx:] set21_phy_by_mode_s7d[188] rterm = 7
[  233.266000] [hdmitx:] Sink is HDMI device
[  233.266172] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  233.266872] [hdmitx:] set audio
[  233.267315] [hdmitx:] audio_param->chs = 1
[  233.267964] [hdmitx:] aud_src_if = 0
[  233.268553] [hdmitx:] aud_n_para = 5120
[  233.269239] [hdmitx:] audio state: AUDIO_UNMUTE
[  233.269873] [hdmitx:] vinfo: set cur_enc_ppc as 1, vpp color: 0
[  233.271000] DOLBY: vout_notify_callback: VOUT_EVENT_MODE_CHANGE
[  233.271631] vsync_pts_inc 3000 1/30
[  233.272365] [drm] meson_vout_update_mode_name: hdmitx update vout 1 name 2160p30hz.
[  233.285555] [snd-soc]: spdif_a is set to disable
[  233.285655] [snd-soc]: aml_audio_reset, reg 0xa, shift 9, use_vadtop 0
[  233.285940] [snd-soc]: aml_audio_reset, reg 0xa, shift 14, use_vadtop 0
[  233.286935] [snd-soc]: hdmitx src switch to spdif 0
[  233.287646] [snd-soc]: sharebuffer_spdifout_prepare  get_hdmitx_audio_src(rtd->card):0  spdif_id:0
[  233.288949] [hdmitx:] hdmitx_audio_notify_callback[798] audio prepare
[  233.289857] [snd-soc]: spdif_a fifo ctrl, frddr:0 type:1, 16 bits, chmask 0x3, swap 0x10
[  233.289874] [hdmitx:] hdmitx_audio_notify_callback[803] type:1 rate:3 size:1 chs:2 i2s_ch_mask:1 aud_src_if:0
[  233.290463] [hdmitx:] hdmitx_set_drm_pkt: tf=16, cf=9, colormetry=0
[  233.291221] [hdmitx:] aout notify format CT_PCM
[  233.291227] [hdmitx:] set audio
[  233.293385] [hdmitx:] audio_param->chs = 1
[  233.294031] [hdmitx:] aud_src_if = 0
[  233.294621] [hdmitx:] aud_n_para = 5120
[  233.295266] [hdmitx:] audio state: AUDIO_UNMUTE
[  233.295949] [hdmitx:] set audio param
[  233.296692] [snd-soc]: spdif_a is set to enable
[  233.320901] [hdmitx:] avmute_store -1
[  234.048154] nf_conntrack: default automatic helper assignment has been turned off for security reasons and CT-based firewall rule not found. Use the iptables CT target to attach helpers instead.
[  238.130578] [hdmitx:] avmute_store 1
[  238.231004] [hdmitx:] phy_store 0
[  238.390777] [drm] build_hdmitx_attr_str:422,12bit = 1+12
[  238.391050] [drm] [meson_hdmitx_encoder_atomic_disable]
[  238.391700] [drm] am_meson_crtc_atomic_disable-[0]:in
[  238.392611] [hdmitx:] hdmitx_set_drm_pkt: disable drm pkt
[  238.393383] [hdmitx:] TV not support DV, clr dv_vsif
[  238.394086] [hdmitx:] DV H14b VSIF, switching signal to SDR
[  238.394976] [hdmitx:] hdmitx_set_hdr10plus_pkt: null vsif
[  238.395849] [hdmitx:] hdmitx_unregister_vrr ret = 0
[  238.396450] [drm] am_meson_crtc_atomic_enable-[0] in: new[1080p50hz], old[2160p30hz], vmode[4-4], uboot[0]
[  238.397826] [drm] am_meson_crtc_atomic_enable-[0]: enable mode 1080p50hz final vmode 0
[  238.399193] [hdmitx:] set21_s7d_htxpll_clk_out[96] htxpll vco 5940000 div 4
[  238.400291] [hdmitx:] pll_od0 = 2, pll_od2 = 1, pll_od1 = 2
[  238.400777] [hdmitx:] clocks_set_vid_clk_div_for_hdmi[402] div = 6
[  238.401685] [hdmitx:] configure venc
[  238.402240] [hdmitx:] config_tv_enc_calc[63] vic = 31
[  238.403022] [hdmitx:] hdmitx_soft_reset[1263]
[  238.403708] [hdmitx:]  config hdmitx IP vic = 31 cd:6 cs: 1
[  238.404523] [hdmitx:] configure hdmitx21
[  238.405174] [hdmitx:] warn: SCDC not present, should not send 1:10
[  238.407219] [hdmitx:] enable phy to dig
[  238.407352] [hdmitx:] hdmitx_set_drm_pkt: tf=1, cf=1, colormetry=0
[  238.407367] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  238.407900] vout changed: 3840x2160->1920x1080
[  238.410609] [hdmitx:] hdmitx_set_dispmode[1551] frl_rate 0 htotal 2640 cs 1 cd 6 h_unstable 0
[  238.448637] [hdmitx:] set21_phy_by_mode_s7d[188] rterm = 7
[  238.449998] [hdmitx:] Sink is HDMI device
[  238.450067] [hdmitx:] clear vsif for non-4k mode.
[  238.450790] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  238.451616] [hdmitx:] set audio
[  238.452048] [hdmitx:] audio_param->chs = 1
[  238.452743] [hdmitx:] aud_src_if = 0
[  238.453288] [hdmitx:] aud_n_para = 6144
[  238.454237] [hdmitx:] audio state: AUDIO_UNMUTE
[  238.454595] [hdmitx:] vinfo: set cur_enc_ppc as 1, vpp color: 0
[  238.455801] DOLBY: vout_notify_callback: VOUT_EVENT_MODE_CHANGE
[  238.456353] vsync_pts_inc 1800 1/50
[  238.457239] [drm] meson_vout_update_mode_name: hdmitx update vout 1 name 1080p50hz.
[  238.460262] [snd-soc]: spdif_a is set to disable
[  238.460339] [snd-soc]: aml_audio_reset, reg 0xa, shift 9, use_vadtop 0
[  238.460651] [snd-soc]: aml_audio_reset, reg 0xa, shift 14, use_vadtop 0
[  238.461616] [snd-soc]: hdmitx src switch to spdif 0
[  238.462324] [snd-soc]: sharebuffer_spdifout_prepare  get_hdmitx_audio_src(rtd->card):0  spdif_id:0
[  238.463601] [hdmitx:] hdmitx_audio_notify_callback[798] audio prepare
[  238.464524] [snd-soc]: spdif_a fifo ctrl, frddr:0 type:1, 16 bits, chmask 0x3, swap 0x10
[  238.464537] [hdmitx:] hdmitx_audio_notify_callback[803] type:1 rate:3 size:1 chs:2 i2s_ch_mask:1 aud_src_if:0
[  238.465924] [hdmitx:] aout notify format CT_PCM
[  238.466606] [hdmitx:] set audio
[  238.467145] [hdmitx:] audio_param->chs = 1
[  238.467354] [hdmitx:] hdmitx_set_drm_pkt: tf=16, cf=9, colormetry=0
[  238.467785] [hdmitx:] aud_src_if = 0
[  238.469297] [hdmitx:] aud_n_para = 6144
[  238.469935] [hdmitx:] audio state: AUDIO_UNMUTE
[  238.470612] [hdmitx:] set audio param
[  238.471306] [snd-soc]: spdif_a is set to enable
[  238.496694] [hdmitx:] avmute_store -1
[  243.094322] [hdmitx:] avmute_store 1
[  243.194602] [hdmitx:] phy_store 0
[  243.327664] [drm] build_hdmitx_attr_str:422,12bit = 1+12
[  243.327889] [drm] [meson_hdmitx_encoder_atomic_disable]
[  243.328604] [drm] am_meson_crtc_atomic_disable-[0]:in
[  243.329491] [hdmitx:] hdmitx_set_drm_pkt: disable drm pkt
[  243.330220] [hdmitx:] TV not support DV, clr dv_vsif
[  243.330972] [hdmitx:] DV H14b VSIF, switching signal to SDR
[  243.331852] [hdmitx:] hdmitx_set_hdr10plus_pkt: null vsif
[  243.332692] [hdmitx:] hdmitx_unregister_vrr ret = 0
[  243.333326] [drm] am_meson_crtc_atomic_enable-[0] in: new[2160p24hz], old[1080p50hz], vmode[4-4], uboot[0]
[  243.334697] [drm] am_meson_crtc_atomic_enable-[0]: enable mode 2160p24hz final vmode 0
[  243.336107] [hdmitx:] set21_s7d_htxpll_clk_out[96] htxpll vco 5940000 div 2
[  243.337205] [hdmitx:] pll_od0 = 1, pll_od2 = 1, pll_od1 = 2
[  243.337635] [hdmitx:] clocks_set_vid_clk_div_for_hdmi[402] div = 6
[  243.338569] [hdmitx:] configure venc
[  243.339125] [hdmitx:] config_tv_enc_calc[63] vic = 93
[  243.339908] [hdmitx:] hdmitx_soft_reset[1263]
[  243.340620] [hdmitx:]  config hdmitx IP vic = 93 cd:6 cs: 1
[  243.341410] [hdmitx:] configure hdmitx21
[  243.342040] [hdmitx:] warn: SCDC not present, should not send 1:10
[  243.344029] [hdmitx:] enable phy to dig
[  243.344084] [hdmitx:] hdmitx_set_dispmode[1551] frl_rate 0 htotal 5500 cs 1 cd 6 h_unstable 0
[  243.344171] [hdmitx:] hdmitx_set_drm_pkt: tf=1, cf=1, colormetry=0
[  243.346097] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  243.347452] vout changed: 1920x1080->3840x2160
[  243.384640] [hdmitx:] set21_phy_by_mode_s7d[188] rterm = 7
[  243.385995] [hdmitx:] Sink is HDMI device
[  243.386204] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  243.386872] [hdmitx:] set audio
[  243.387314] [hdmitx:] audio_param->chs = 1
[  243.387962] [hdmitx:] aud_src_if = 0
[  243.388597] [hdmitx:] aud_n_para = 5120
[  243.389211] [hdmitx:] audio state: AUDIO_UNMUTE
[  243.389871] [hdmitx:] vinfo: set cur_enc_ppc as 1, vpp color: 0
[  243.391030] DOLBY: vout_notify_callback: VOUT_EVENT_MODE_CHANGE
[  243.391631] vsync_pts_inc 3750 1/24
[  243.392401] [drm] meson_vout_update_mode_name: hdmitx update vout 1 name 2160p24hz.
[  243.410748] [snd-soc]: spdif_a is set to disable
[  243.410847] [snd-soc]: aml_audio_reset, reg 0xa, shift 9, use_vadtop 0
[  243.411132] [snd-soc]: aml_audio_reset, reg 0xa, shift 14, use_vadtop 0
[  243.412126] [snd-soc]: hdmitx src switch to spdif 0
[  243.412865] [snd-soc]: sharebuffer_spdifout_prepare  get_hdmitx_audio_src(rtd->card):0  spdif_id:0
[  243.414118] [hdmitx:] hdmitx_audio_notify_callback[798] audio prepare
[  243.415040] [snd-soc]: spdif_a fifo ctrl, frddr:0 type:1, 16 bits, chmask 0x3, swap 0x10
[  243.415057] [hdmitx:] hdmitx_audio_notify_callback[803] type:1 rate:3 size:1 chs:2 i2s_ch_mask:1 aud_src_if:0
[  243.416415] [hdmitx:] aout notify format CT_PCM
[  243.417161] [hdmitx:] set audio
[  243.417662] [hdmitx:] audio_param->chs = 1
[  243.418302] [hdmitx:] aud_src_if = 0
[  243.418892] [hdmitx:] aud_n_para = 5120
[  243.419550] [hdmitx:] audio state: AUDIO_UNMUTE
[  243.420227] [hdmitx:] set audio param
[  243.420956] [snd-soc]: spdif_a is set to enable
[  243.427499] [hdmitx:] hdmitx_set_drm_pkt: tf=16, cf=9, colormetry=0
[  243.452163] [hdmitx:] avmute_store -1
[  248.144028] [hdmitx:] avmute_store 1
[  248.244370] [hdmitx:] phy_store 0
[  248.386079] [drm] [meson_encoder_vrr_change], seamless is 0
[  248.386251] [drm] build_hdmitx_attr_str:422,12bit = 1+12
[  248.387140] [drm] [meson_hdmitx_encoder_atomic_disable]
[  248.387840] [drm] am_meson_crtc_atomic_disable-[0]:in
[  248.388782] [hdmitx:] hdmitx_set_drm_pkt: disable drm pkt
[  248.389521] [hdmitx:] TV not support DV, clr dv_vsif
[  248.390226] [hdmitx:] DV H14b VSIF, switching signal to SDR
[  248.391106] [hdmitx:] hdmitx_set_hdr10plus_pkt: null vsif
[  248.391950] [hdmitx:] hdmitx_unregister_vrr ret = 0
[  248.392621] [drm] am_meson_crtc_atomic_enable-[0] in: new[2160p30hz], old[2160p24hz], vmode[4-4], uboot[0]
[  248.393947] [drm] am_meson_crtc_atomic_enable-[0]: enable mode 2160p30hz final vmode 0
[  248.395376] [hdmitx:] set21_s7d_htxpll_clk_out[96] htxpll vco 5940000 div 2
[  248.396426] [hdmitx:] pll_od0 = 1, pll_od2 = 1, pll_od1 = 2
[  248.396924] [hdmitx:] clocks_set_vid_clk_div_for_hdmi[402] div = 6
[  248.397826] [hdmitx:] configure venc
[  248.398380] [hdmitx:] config_tv_enc_calc[63] vic = 95
[  248.399162] [hdmitx:] hdmitx_soft_reset[1263]
[  248.399848] [hdmitx:]  config hdmitx IP vic = 95 cd:6 cs: 1
[  248.400686] [hdmitx:] configure hdmitx21
[  248.401296] [hdmitx:] warn: SCDC not present, should not send 1:10
[  248.403280] [hdmitx:] enable phy to dig
[  248.403332] [hdmitx:] hdmitx_set_dispmode[1551] frl_rate 0 htotal 4400 cs 1 cd 6 h_unstable 0
[  248.403406] [hdmitx:] hdmitx_set_drm_pkt: tf=1, cf=1, colormetry=0
[  248.405347] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  248.440647] [hdmitx:] set21_phy_by_mode_s7d[188] rterm = 7
[  248.441967] [hdmitx:] Sink is HDMI device
[  248.442107] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  248.442846] [hdmitx:] set audio
[  248.443281] [hdmitx:] audio_param->chs = 1
[  248.443926] [hdmitx:] aud_src_if = 0
[  248.444515] [hdmitx:] aud_n_para = 5120
[  248.445259] [hdmitx:] audio state: AUDIO_UNMUTE
[  248.445839] [hdmitx:] vinfo: set cur_enc_ppc as 1, vpp color: 0
[  248.446935] DOLBY: vout_notify_callback: VOUT_EVENT_MODE_CHANGE
[  248.447595] vsync_pts_inc 3000 1/30
[  248.448307] [drm] meson_vout_update_mode_name: hdmitx update vout 1 name 2160p30hz.
[  248.457789] [snd-soc]: spdif_a is set to disable
[  248.457866] [snd-soc]: aml_audio_reset, reg 0xa, shift 9, use_vadtop 0
[  248.458144] [snd-soc]: aml_audio_reset, reg 0xa, shift 14, use_vadtop 0
[  248.459138] [snd-soc]: hdmitx src switch to spdif 0
[  248.459852] [snd-soc]: sharebuffer_spdifout_prepare  get_hdmitx_audio_src(rtd->card):0  spdif_id:0
[  248.461151] [hdmitx:] hdmitx_audio_notify_callback[798] audio prepare
[  248.462053] [snd-soc]: spdif_a fifo ctrl, frddr:0 type:1, 16 bits, chmask 0x3, swap 0x10
[  248.462066] [hdmitx:] hdmitx_audio_notify_callback[803] type:1 rate:3 size:1 chs:2 i2s_ch_mask:1 aud_src_if:0
[  248.463426] [hdmitx:] aout notify format CT_PCM
[  248.464130] [hdmitx:] set audio
[  248.464677] [hdmitx:] audio_param->chs = 1
[  248.465315] [hdmitx:] aud_src_if = 0
[  248.465902] [hdmitx:] aud_n_para = 5120
[  248.466544] [hdmitx:] audio state: AUDIO_UNMUTE
[  248.467249] [hdmitx:] set audio param
[  248.467913] [snd-soc]: spdif_a is set to enable
[  248.470100] [hdmitx:] hdmitx_set_drm_pkt: tf=16, cf=9, colormetry=0
[  248.495389] [hdmitx:] avmute_store -1
[  254.842090] [hdmitx:] avmute_store 1
[  254.942356] [hdmitx:] phy_store 0
[  255.103687] [drm] [meson_encoder_vrr_change], seamless is 0
[  255.103863] [drm] build_hdmitx_attr_str:422,12bit = 1+12
[  255.104786] [drm] [meson_hdmitx_encoder_atomic_disable]
[  255.105452] [drm] am_meson_crtc_atomic_disable-[0]:in
[  255.106368] [hdmitx:] hdmitx_set_drm_pkt: disable drm pkt
[  255.107161] [hdmitx:] TV not support DV, clr dv_vsif
[  255.107852] [hdmitx:] DV H14b VSIF, switching signal to SDR
[  255.108772] [hdmitx:] hdmitx_set_hdr10plus_pkt: null vsif
[  255.109562] [hdmitx:] hdmitx_unregister_vrr ret = 0
[  255.110191] [drm] am_meson_crtc_atomic_enable-[0] in: new[2160p25hz], old[2160p30hz], vmode[4-4], uboot[0]
[  255.111550] [drm] am_meson_crtc_atomic_enable-[0]: enable mode 2160p25hz final vmode 0
[  255.112956] [hdmitx:] set21_s7d_htxpll_clk_out[96] htxpll vco 5940000 div 2
[  255.114010] [hdmitx:] pll_od0 = 1, pll_od2 = 1, pll_od1 = 2
[  255.114499] [hdmitx:] clocks_set_vid_clk_div_for_hdmi[402] div = 6
[  255.115428] [hdmitx:] configure venc
[  255.115989] [hdmitx:] config_tv_enc_calc[63] vic = 94
[  255.116788] [hdmitx:] hdmitx_soft_reset[1263]
[  255.117455] [hdmitx:]  config hdmitx IP vic = 94 cd:6 cs: 1
[  255.118277] [hdmitx:] configure hdmitx21
[  255.118904] [hdmitx:] warn: SCDC not present, should not send 1:10
[  255.120879] [hdmitx:] enable phy to dig
[  255.120926] [hdmitx:] hdmitx_set_dispmode[1551] frl_rate 0 htotal 5280 cs 1 cd 6 h_unstable 0
[  255.121009] [hdmitx:] hdmitx_set_drm_pkt: tf=1, cf=1, colormetry=0
[  255.122937] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  255.164649] [hdmitx:] set21_phy_by_mode_s7d[188] rterm = 7
[  255.166007] [hdmitx:] Sink is HDMI device
[  255.166211] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  255.166882] [hdmitx:] set audio
[  255.167324] [hdmitx:] audio_param->chs = 1
[  255.167972] [hdmitx:] aud_src_if = 0
[  255.168562] [hdmitx:] aud_n_para = 5120
[  255.169220] [hdmitx:] audio state: AUDIO_UNMUTE
[  255.169881] [hdmitx:] vinfo: set cur_enc_ppc as 1, vpp color: 0
[  255.170987] DOLBY: vout_notify_callback: VOUT_EVENT_MODE_CHANGE
[  255.171642] vsync_pts_inc 3600 1/25
[  255.172409] [drm] meson_vout_update_mode_name: hdmitx update vout 1 name 2160p25hz.
[  255.200937] [snd-soc]: spdif_a is set to disable
[  255.200996] [snd-soc]: aml_audio_reset, reg 0xa, shift 9, use_vadtop 0
[  255.201016] [hdmitx:] hdmitx_set_drm_pkt: tf=16, cf=9, colormetry=0
[  255.201270] [snd-soc]: aml_audio_reset, reg 0xa, shift 14, use_vadtop 0
[  255.203266] [snd-soc]: hdmitx src switch to spdif 0
[  255.203901] [snd-soc]: sharebuffer_spdifout_prepare  get_hdmitx_audio_src(rtd->card):0  spdif_id:0
[  255.205253] [hdmitx:] hdmitx_audio_notify_callback[798] audio prepare
[  255.206116] [snd-soc]: spdif_a fifo ctrl, frddr:0 type:1, 16 bits, chmask 0x3, swap 0x10
[  255.206129] [hdmitx:] hdmitx_audio_notify_callback[803] type:1 rate:3 size:1 chs:2 i2s_ch_mask:1 aud_src_if:0
[  255.207475] [hdmitx:] aout notify format CT_PCM
[  255.208177] [hdmitx:] set audio
[  255.208727] [hdmitx:] audio_param->chs = 1
[  255.209360] [hdmitx:] aud_src_if = 0
[  255.209949] [hdmitx:] aud_n_para = 5120
[  255.210587] [hdmitx:] audio state: AUDIO_UNMUTE
[  255.211294] [hdmitx:] set audio param
[  255.211973] [snd-soc]: spdif_a is set to enable
[  255.226237] [hdmitx:] avmute_store -1
[  258.765862] [hdmitx:] avmute_store 1
[  258.866167] [hdmitx:] phy_store 0
[  259.001255] [drm] [meson_encoder_vrr_change], seamless is 0
[  259.001433] [drm] build_hdmitx_attr_str:422,12bit = 1+12
[  259.002333] [drm] [meson_hdmitx_encoder_atomic_disable]
[  259.003039] [drm] am_meson_crtc_atomic_disable-[0]:in
[  259.003937] [hdmitx:] hdmitx_set_drm_pkt: disable drm pkt
[  259.004810] [hdmitx:] TV not support DV, clr dv_vsif
[  259.005433] [hdmitx:] DV H14b VSIF, switching signal to SDR
[  259.006346] [hdmitx:] hdmitx_set_hdr10plus_pkt: null vsif
[  259.007134] [hdmitx:] hdmitx_unregister_vrr ret = 0
[  259.007769] [drm] am_meson_crtc_atomic_enable-[0] in: new[2160p30hz], old[2160p25hz], vmode[4-4], uboot[0]
[  259.009586] [drm] am_meson_crtc_atomic_enable-[0]: enable mode 2160p30hz final vmode 0
[  259.010567] [hdmitx:] set21_s7d_htxpll_clk_out[96] htxpll vco 5940000 div 2
[  259.011600] [hdmitx:] pll_od0 = 1, pll_od2 = 1, pll_od1 = 2
[  259.012069] [hdmitx:] clocks_set_vid_clk_div_for_hdmi[402] div = 6
[  259.013027] [hdmitx:] configure venc
[  259.013560] [hdmitx:] config_tv_enc_calc[63] vic = 95
[  259.014339] [hdmitx:] hdmitx_soft_reset[1263]
[  259.015023] [hdmitx:]  config hdmitx IP vic = 95 cd:6 cs: 1
[  259.015844] [hdmitx:] configure hdmitx21
[  259.016473] [hdmitx:] warn: SCDC not present, should not send 1:10
[  259.018486] [hdmitx:] enable phy to dig
[  259.018528] [hdmitx:] hdmitx_set_dispmode[1551] frl_rate 0 htotal 4400 cs 1 cd 6 h_unstable 0
[  259.018610] [hdmitx:] hdmitx_set_drm_pkt: tf=1, cf=1, colormetry=0
[  259.020543] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  259.056644] [hdmitx:] set21_phy_by_mode_s7d[188] rterm = 7
[  259.057980] [hdmitx:] Sink is HDMI device
[  259.058146] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  259.058832] [hdmitx:] set audio
[  259.059295] [hdmitx:] audio_param->chs = 1
[  259.059943] [hdmitx:] aud_src_if = 0
[  259.060532] [hdmitx:] aud_n_para = 5120
[  259.061204] [hdmitx:] audio state: AUDIO_UNMUTE
[  259.061853] [hdmitx:] vinfo: set cur_enc_ppc as 1, vpp color: 0
[  259.063012] DOLBY: vout_notify_callback: VOUT_EVENT_MODE_CHANGE
[  259.063613] vsync_pts_inc 3000 1/30
[  259.064384] [drm] meson_vout_update_mode_name: hdmitx update vout 1 name 2160p30hz.
[  259.065085] [snd-soc]: spdif_a is set to disable
[  259.065350] [snd-soc]: aml_audio_reset, reg 0xa, shift 9, use_vadtop 0
[  259.066231] [snd-soc]: aml_audio_reset, reg 0xa, shift 14, use_vadtop 0
[  259.067229] [snd-soc]: hdmitx src switch to spdif 0
[  259.067937] [snd-soc]: sharebuffer_spdifout_prepare  get_hdmitx_audio_src(rtd->card):0  spdif_id:0
[  259.069259] [hdmitx:] hdmitx_audio_notify_callback[798] audio prepare
[  259.070138] [snd-soc]: spdif_a fifo ctrl, frddr:0 type:1, 16 bits, chmask 0x3, swap 0x10
[  259.070155] [hdmitx:] hdmitx_audio_notify_callback[803] type:1 rate:3 size:1 chs:2 i2s_ch_mask:1 aud_src_if:0
[  259.071511] [hdmitx:] aout notify format CT_PCM
[  259.072215] [hdmitx:] set audio
[  259.072775] [hdmitx:] audio_param->chs = 1
[  259.073398] [hdmitx:] aud_src_if = 0
[  259.073987] [hdmitx:] aud_n_para = 5120
[  259.074631] [hdmitx:] audio state: AUDIO_UNMUTE
[  259.075319] [hdmitx:] set audio param
[  259.076001] [snd-soc]: spdif_a is set to enable
[  259.085298] [hdmitx:] hdmitx_set_drm_pkt: tf=16, cf=9, colormetry=0
[  259.110723] [hdmitx:] avmute_store -1
[  263.144639] [aml_send_sync_trace 4388] sync token[36942]
[  263.144661] >>> aml_send_msg()
[  263.145588] ipc_sdio_host_msgack_handler 00000000c10cd5bf
[  263.146115] [aml_msgackind 2039] msg ack hostid=0xffffff80799b8400
[  263.147021] [cmd_mgr_llind         329] cmd tkn[41]  flags:0008  result: -4  cmd: 105-MM_SYNC_TRACE            - reqcfm(   0-none)
[  263.148643] [cmd_complete           65] cmd tkn[41]  flags:0000  result: -4  cmd: 105-MM_SYNC_TRACE            - reqcfm(   0-none)
[  263.326397] [hdmitx:] avmute_store 1
[  263.426695] [hdmitx:] phy_store 0
[  263.585513] [drm] [meson_encoder_vrr_change], seamless is 0
[  263.585684] [drm] build_hdmitx_attr_str:422,12bit = 1+12
[  263.586574] [drm] [meson_hdmitx_encoder_atomic_disable]
[  263.587272] [drm] am_meson_crtc_atomic_disable-[0]:in
[  263.588191] [hdmitx:] hdmitx_set_drm_pkt: disable drm pkt
[  263.589017] [hdmitx:] TV not support DV, clr dv_vsif
[  263.589677] [hdmitx:] DV H14b VSIF, switching signal to SDR
[  263.590583] [hdmitx:] hdmitx_set_hdr10plus_pkt: null vsif
[  263.591383] [hdmitx:] hdmitx_unregister_vrr ret = 0
[  263.592015] [drm] am_meson_crtc_atomic_enable-[0] in: new[2160p25hz], old[2160p30hz], vmode[4-4], uboot[0]
[  263.593401] [drm] am_meson_crtc_atomic_enable-[0]: enable mode 2160p25hz final vmode 0
[  263.594804] [hdmitx:] set21_s7d_htxpll_clk_out[96] htxpll vco 5940000 div 2
[  263.595875] [hdmitx:] pll_od0 = 1, pll_od2 = 1, pll_od1 = 2
[  263.596323] [hdmitx:] clocks_set_vid_clk_div_for_hdmi[402] div = 6
[  263.597281] [hdmitx:] configure venc
[  263.597813] [hdmitx:] config_tv_enc_calc[63] vic = 94
[  263.598593] [hdmitx:] hdmitx_soft_reset[1263]
[  263.599276] [hdmitx:]  config hdmitx IP vic = 94 cd:6 cs: 1
[  263.600163] [hdmitx:] configure hdmitx21
[  263.600765] [hdmitx:] warn: SCDC not present, should not send 1:10
[  263.602706] [hdmitx:] enable phy to dig
[  263.602743] [hdmitx:] hdmitx_set_dispmode[1551] frl_rate 0 htotal 5280 cs 1 cd 6 h_unstable 0
[  263.602835] [hdmitx:] hdmitx_set_drm_pkt: tf=1, cf=1, colormetry=0
[  263.604758] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  263.644673] [hdmitx:] set21_phy_by_mode_s7d[188] rterm = 7
[  263.646029] [hdmitx:] Sink is HDMI device
[  263.646210] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  263.646893] [hdmitx:] set audio
[  263.647356] [hdmitx:] audio_param->chs = 1
[  263.648004] [hdmitx:] aud_src_if = 0
[  263.648618] [hdmitx:] aud_n_para = 5120
[  263.649301] [hdmitx:] audio state: AUDIO_UNMUTE
[  263.649918] [hdmitx:] vinfo: set cur_enc_ppc as 1, vpp color: 0
[  263.651036] DOLBY: vout_notify_callback: VOUT_EVENT_MODE_CHANGE
[  263.651672] vsync_pts_inc 3600 1/25
[  263.652443] [drm] meson_vout_update_mode_name: hdmitx update vout 1 name 2160p25hz.
[  263.664892] [snd-soc]: spdif_a is set to disable
[  263.664949] [snd-soc]: aml_audio_reset, reg 0xa, shift 9, use_vadtop 0
[  263.665222] [snd-soc]: aml_audio_reset, reg 0xa, shift 14, use_vadtop 0
[  263.666209] [snd-soc]: hdmitx src switch to spdif 0
[  263.666930] [snd-soc]: sharebuffer_spdifout_prepare  get_hdmitx_audio_src(rtd->card):0  spdif_id:0
[  263.668203] [hdmitx:] hdmitx_audio_notify_callback[798] audio prepare
[  263.669164] [snd-soc]: spdif_a fifo ctrl, frddr:0 type:1, 16 bits, chmask 0x3, swap 0x10
[  263.669177] [hdmitx:] hdmitx_audio_notify_callback[803] type:1 rate:3 size:1 chs:2 i2s_ch_mask:1 aud_src_if:0
[  263.670507] [hdmitx:] aout notify format CT_PCM
[  263.671209] [hdmitx:] set audio
[  263.671748] [hdmitx:] audio_param->chs = 1
[  263.672393] [hdmitx:] aud_src_if = 0
[  263.673030] [hdmitx:] aud_n_para = 5120
[  263.673619] [hdmitx:] audio state: AUDIO_UNMUTE
[  263.674309] [hdmitx:] set audio param
[  263.674987] [snd-soc]: spdif_a is set to enable
[  263.682840] [hdmitx:] hdmitx_set_drm_pkt: tf=16, cf=9, colormetry=0
[  263.708664] [hdmitx:] avmute_store -1
[  267.611645] [hdmitx:] avmute_store 1
[  267.711883] [hdmitx:] phy_store 0
[  267.883061] [drm] [meson_encoder_vrr_change], seamless is 0
[  267.883231] [drm] build_hdmitx_attr_str:422,12bit = 1+12
[  267.884116] [drm] [meson_hdmitx_encoder_atomic_disable]
[  267.885102] [drm] am_meson_crtc_atomic_disable-[0]:in
[  267.885761] [hdmitx:] hdmitx_set_drm_pkt: disable drm pkt
[  267.886517] [hdmitx:] TV not support DV, clr dv_vsif
[  267.887208] [hdmitx:] DV H14b VSIF, switching signal to SDR
[  267.888087] [hdmitx:] hdmitx_set_hdr10plus_pkt: null vsif
[  267.888926] [hdmitx:] hdmitx_unregister_vrr ret = 0
[  267.889562] [drm] am_meson_crtc_atomic_enable-[0] in: new[2160p30hz], old[2160p25hz], vmode[4-4], uboot[0]
[  267.890925] [drm] am_meson_crtc_atomic_enable-[0]: enable mode 2160p30hz final vmode 0
[  267.892306] [hdmitx:] set21_s7d_htxpll_clk_out[96] htxpll vco 5940000 div 2
[  267.893441] [hdmitx:] pll_od0 = 1, pll_od2 = 1, pll_od1 = 2
[  267.893870] [hdmitx:] clocks_set_vid_clk_div_for_hdmi[402] div = 6
[  267.895016] [hdmitx:] configure venc
[  267.895379] [hdmitx:] config_tv_enc_calc[63] vic = 95
[  267.896142] [hdmitx:] hdmitx_soft_reset[1263]
[  267.896859] [hdmitx:]  config hdmitx IP vic = 95 cd:6 cs: 1
[  267.897661] [hdmitx:] configure hdmitx21
[  267.898275] [hdmitx:] warn: SCDC not present, should not send 1:10
[  267.900318] [hdmitx:] enable phy to dig
[  267.900373] [hdmitx:] hdmitx_set_dispmode[1551] frl_rate 0 htotal 4400 cs 1 cd 6 h_unstable 0
[  267.900446] [hdmitx:] hdmitx_set_drm_pkt: tf=1, cf=1, colormetry=0
[  267.902384] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  267.940653] [hdmitx:] set21_phy_by_mode_s7d[188] rterm = 7
[  267.941967] [hdmitx:] Sink is HDMI device
[  267.942089] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  267.942860] [hdmitx:] set audio
[  267.943276] [hdmitx:] audio_param->chs = 1
[  267.943922] [hdmitx:] aud_src_if = 0
[  267.944512] [hdmitx:] aud_n_para = 5120
[  267.945203] [hdmitx:] audio state: AUDIO_UNMUTE
[  267.945832] [hdmitx:] vinfo: set cur_enc_ppc as 1, vpp color: 0
[  267.946956] DOLBY: vout_notify_callback: VOUT_EVENT_MODE_CHANGE
[  267.947591] vsync_pts_inc 3000 1/30
[  267.948422] [drm] meson_vout_update_mode_name: hdmitx update vout 1 name 2160p30hz.
[  267.967140] [hdmitx:] hdmitx_set_drm_pkt: tf=16, cf=9, colormetry=0
[  267.976047] [snd-soc]: spdif_a is set to disable
[  267.976133] [snd-soc]: aml_audio_reset, reg 0xa, shift 9, use_vadtop 0
[  267.976416] [snd-soc]: aml_audio_reset, reg 0xa, shift 14, use_vadtop 0
[  267.977447] [snd-soc]: hdmitx src switch to spdif 0
[  267.978123] [snd-soc]: sharebuffer_spdifout_prepare  get_hdmitx_audio_src(rtd->card):0  spdif_id:0
[  267.979397] [hdmitx:] hdmitx_audio_notify_callback[798] audio prepare
[  267.980322] [snd-soc]: spdif_a fifo ctrl, frddr:0 type:1, 16 bits, chmask 0x3, swap 0x10
[  267.980336] [hdmitx:] hdmitx_audio_notify_callback[803] type:1 rate:3 size:1 chs:2 i2s_ch_mask:1 aud_src_if:0
[  267.981718] [hdmitx:] aout notify format CT_PCM
[  267.982401] [hdmitx:] set audio
[  267.982939] [hdmitx:] audio_param->chs = 1
[  267.983585] [hdmitx:] aud_src_if = 0
[  267.984173] [hdmitx:] aud_n_para = 5120
[  267.984832] [hdmitx:] audio state: AUDIO_UNMUTE
[  267.985503] [hdmitx:] set audio param
[  267.986178] [snd-soc]: spdif_a is set to enable
[  267.993029] [hdmitx:] avmute_store -1
[  271.610266] [hdmitx:] avmute_store 1
[  271.710668] [hdmitx:] phy_store 0
[  271.867467] [drm] build_hdmitx_attr_str:420,8bit = 3+8
[  271.867695] [drm] [meson_hdmitx_encoder_atomic_disable]
[  271.868372] [drm] am_meson_crtc_atomic_disable-[0]:in
[  271.869538] [hdmitx:] hdmitx_set_drm_pkt: disable drm pkt
[  271.870096] [hdmitx:] TV not support DV, clr dv_vsif
[  271.870770] [hdmitx:] DV H14b VSIF, switching signal to SDR
[  271.871655] [hdmitx:] hdmitx_set_hdr10plus_pkt: null vsif
[  271.872453] [hdmitx:] hdmitx_unregister_vrr ret = 0
[  271.873152] [drm] am_meson_crtc_atomic_enable-[0] in: new[2160p50hz], old[2160p30hz], vmode[4-4], uboot[0]
[  271.874492] [drm] am_meson_crtc_atomic_enable-[0]: enable mode 2160p50hz final vmode 0
[  271.875850] [hdmitx:] set21_s7d_htxpll_clk_out[96] htxpll vco 5940000 div 2
[  271.876961] [hdmitx:] pll_od0 = 1, pll_od2 = 0, pll_od1 = 0
[  271.877421] [hdmitx:] clocks_set_vid_clk_div_for_hdmi[402] div = 6
[  271.878352] [hdmitx:] configure venc
[  271.878910] [hdmitx:] config_tv_enc_calc[63] vic = 96
[  271.879717] [hdmitx:] hdmitx_soft_reset[1263]
[  271.880374] [hdmitx:]  config hdmitx IP vic = 96 cd:4 cs: 3
[  271.881219] [hdmitx:] configure hdmitx21
[  271.881828] [hdmitx:] warn: SCDC not present, should not send 1:10
[  271.883814] [hdmitx:] enable phy to dig
[  271.883870] [hdmitx:] hdmitx_set_dispmode[1551] frl_rate 0 htotal 5280 cs 3 cd 4 h_unstable 0
[  271.883947] [hdmitx:] hdmitx_set_drm_pkt: tf=1, cf=1, colormetry=0
[  271.885883] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  271.924649] [hdmitx:] set21_phy_by_mode_s7d[188] rterm = 7
[  271.926007] [hdmitx:] Sink is HDMI device
[  271.926078] [hdmitx:] clear vsif for non-4k mode.
[  271.926730] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  271.927608] [hdmitx:] set audio
[  271.928049] [hdmitx:] audio_param->chs = 1
[  271.928722] [hdmitx:] aud_src_if = 0
[  271.929288] [hdmitx:] aud_n_para = 5120
[  271.929944] [hdmitx:] audio state: AUDIO_UNMUTE
[  271.930607] [hdmitx:] vinfo: set cur_enc_ppc as 1, vpp color: 0
[  271.931751] DOLBY: vout_notify_callback: VOUT_EVENT_MODE_CHANGE
[  271.932366] vsync_pts_inc 1800 1/50
[  271.933183] [drm] meson_vout_update_mode_name: hdmitx update vout 1 name 2160p50hz.
[  271.935438] [snd-soc]: spdif_a is set to disable
[  271.935507] [snd-soc]: aml_audio_reset, reg 0xa, shift 9, use_vadtop 0
[  271.935784] [snd-soc]: aml_audio_reset, reg 0xa, shift 14, use_vadtop 0
[  271.936814] [snd-soc]: hdmitx src switch to spdif 0
[  271.937494] [snd-soc]: sharebuffer_spdifout_prepare  get_hdmitx_audio_src(rtd->card):0  spdif_id:0
[  271.938763] [hdmitx:] hdmitx_audio_notify_callback[798] audio prepare
[  271.939691] [snd-soc]: spdif_a fifo ctrl, frddr:0 type:1, 16 bits, chmask 0x3, swap 0x10
[  271.939702] [hdmitx:] hdmitx_audio_notify_callback[803] type:1 rate:3 size:1 chs:2 i2s_ch_mask:1 aud_src_if:0
[  271.941085] [hdmitx:] aout notify format CT_PCM
[  271.941770] [hdmitx:] set audio
[  271.942310] [hdmitx:] audio_param->chs = 1
[  271.942953] [hdmitx:] aud_src_if = 0
[  271.943543] [hdmitx:] aud_n_para = 5120
[  271.944184] [hdmitx:] audio state: AUDIO_UNMUTE
[  271.944885] [hdmitx:] set audio param
[  271.945563] [snd-soc]: spdif_a is set to enable
[  271.967314] [hdmitx:] avmute_store -1
[  275.769618] [hdmitx:] avmute_store 1
[  275.869902] [hdmitx:] phy_store 0
[  276.004269] [drm] build_hdmitx_attr_str:422,12bit = 1+12
[  276.004497] [drm] [meson_hdmitx_encoder_atomic_disable]
[  276.005213] [drm] am_meson_crtc_atomic_disable-[0]:in
[  276.006072] [hdmitx:] hdmitx_set_drm_pkt: disable drm pkt
[  276.006825] [hdmitx:] TV not support DV, clr dv_vsif
[  276.007577] [hdmitx:] DV H14b VSIF, switching signal to SDR
[  276.008459] [hdmitx:] hdmitx_set_hdr10plus_pkt: null vsif
[  276.009488] [hdmitx:] hdmitx_unregister_vrr ret = 0
[  276.009952] [drm] am_meson_crtc_atomic_enable-[0] in: new[2160p30hz], old[2160p50hz], vmode[4-4], uboot[0]
[  276.011315] [drm] am_meson_crtc_atomic_enable-[0]: enable mode 2160p30hz final vmode 0
[  276.012837] [hdmitx:] set21_s7d_htxpll_clk_out[96] htxpll vco 5940000 div 2
[  276.013801] [hdmitx:] pll_od0 = 1, pll_od2 = 1, pll_od1 = 2
[  276.014240] [hdmitx:] clocks_set_vid_clk_div_for_hdmi[402] div = 6
[  276.015175] [hdmitx:] configure venc
[  276.015731] [hdmitx:] config_tv_enc_calc[63] vic = 95
[  276.016512] [hdmitx:] hdmitx_soft_reset[1263]
[  276.017255] [hdmitx:]  config hdmitx IP vic = 95 cd:6 cs: 1
[  276.018040] [hdmitx:] configure hdmitx21
[  276.018646] [hdmitx:] warn: SCDC not present, should not send 1:10
[  276.020627] [hdmitx:] enable phy to dig
[  276.020878] [hdmitx:] hdmitx_set_dispmode[1551] frl_rate 0 htotal 4400 cs 1 cd 6 h_unstable 0
[  276.064665] [hdmitx:] set21_phy_by_mode_s7d[188] rterm = 7
[  276.066009] [hdmitx:] Sink is HDMI device
[  276.066161] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  276.066870] [hdmitx:] set audio
[  276.067332] [hdmitx:] audio_param->chs = 1
[  276.067981] [hdmitx:] aud_src_if = 0
[  276.068587] [hdmitx:] aud_n_para = 5120
[  276.069220] [hdmitx:] audio state: AUDIO_UNMUTE
[  276.069890] [hdmitx:] vinfo: set cur_enc_ppc as 1, vpp color: 0
[  276.071018] DOLBY: vout_notify_callback: VOUT_EVENT_MODE_CHANGE
[  276.071650] vsync_pts_inc 3000 1/30
[  276.072395] [drm] meson_vout_update_mode_name: hdmitx update vout 1 name 2160p30hz.
[  276.086165] [snd-soc]: spdif_a is set to disable
[  276.086260] [snd-soc]: aml_audio_reset, reg 0xa, shift 9, use_vadtop 0
[  276.086542] [snd-soc]: aml_audio_reset, reg 0xa, shift 14, use_vadtop 0
[  276.087445] [hdmitx:] hdmitx_set_drm_pkt: tf=16, cf=9, colormetry=0
[  276.087535] [snd-soc]: hdmitx src switch to spdif 0
[  276.089201] [snd-soc]: sharebuffer_spdifout_prepare  get_hdmitx_audio_src(rtd->card):0  spdif_id:0
[  276.090442] [hdmitx:] hdmitx_audio_notify_callback[798] audio prepare
[  276.091370] [snd-soc]: spdif_a fifo ctrl, frddr:0 type:1, 16 bits, chmask 0x3, swap 0x10
[  276.091383] [hdmitx:] hdmitx_audio_notify_callback[803] type:1 rate:3 size:1 chs:2 i2s_ch_mask:1 aud_src_if:0
[  276.092763] [hdmitx:] aout notify format CT_PCM
[  276.093449] [hdmitx:] set audio
[  276.093988] [hdmitx:] audio_param->chs = 1
[  276.094632] [hdmitx:] aud_src_if = 0
[  276.095221] [hdmitx:] aud_n_para = 5120
[  276.095868] [hdmitx:] audio state: AUDIO_UNMUTE
[  276.096553] [hdmitx:] set audio param
[  276.097264] [snd-soc]: spdif_a is set to enable
[  276.116869] [hdmitx:] avmute_store -1
[  276.183691] [SP FRAME RX] arp req,vif_idx:0 sender:[f8:8c:21:8f:40:25 192.168.0.1]receiver:[00:00:00:00:00:00 192.168.0.108]
[  276.184645] [SP FRAME TX] arp rsp,vif_idx:0 sender:[c0:e3:50:49:af:ae 192.168.0.108]receiver:[f8:8c:21:8f:40:25 192.168.0.1]
[  276.200667] [SP FRAME TX] arp req,vif_idx:0 sender:[c0:e3:50:49:af:ae 192.168.0.108]receiver:[00:00:00:00:00:00 192.168.0.1]
[  276.204481] [SP FRAME RX] arp rsp,vif_idx:0 sender:[f8:8c:21:8f:40:25 192.168.0.1]receiver:[c0:e3:50:49:af:ae 192.168.0.108]
[  276.750575] [SP FRAME RX] DHCP[1 0], vif_idx:0
[  279.830159] [hdmitx:] avmute_store 1
[  279.930423] [hdmitx:] phy_store 0
[  280.087822] [drm] [meson_encoder_vrr_change], seamless is 0
[  280.087998] [drm] build_hdmitx_attr_str:422,12bit = 1+12
[  280.088959] [drm] [meson_hdmitx_encoder_atomic_disable]
[  280.089614] [drm] am_meson_crtc_atomic_disable-[0]:in
[  280.090503] [hdmitx:] hdmitx_set_drm_pkt: disable drm pkt
[  280.091299] [hdmitx:] TV not support DV, clr dv_vsif
[  280.091987] [hdmitx:] DV H14b VSIF, switching signal to SDR
[  280.092899] [hdmitx:] hdmitx_set_hdr10plus_pkt: null vsif
[  280.093697] [hdmitx:] hdmitx_unregister_vrr ret = 0
[  280.094329] [drm] am_meson_crtc_atomic_enable-[0] in: new[2160p25hz], old[2160p30hz], vmode[4-4], uboot[0]
[  280.095690] [drm] am_meson_crtc_atomic_enable-[0]: enable mode 2160p25hz final vmode 0
[  280.097163] [hdmitx:] set21_s7d_htxpll_clk_out[96] htxpll vco 5940000 div 2
[  280.098533] [hdmitx:] pll_od0 = 1, pll_od2 = 1, pll_od1 = 2
[  280.098689] [hdmitx:] clocks_set_vid_clk_div_for_hdmi[402] div = 6
[  280.099616] [hdmitx:] configure venc
[  280.100180] [hdmitx:] config_tv_enc_calc[63] vic = 94
[  280.101007] [hdmitx:] hdmitx_soft_reset[1263]
[  280.101644] [hdmitx:]  config hdmitx IP vic = 94 cd:6 cs: 1
[  280.102463] [hdmitx:] configure hdmitx21
[  280.103093] [hdmitx:] warn: SCDC not present, should not send 1:10
[  280.105057] [hdmitx:] enable phy to dig
[  280.105180] [hdmitx:] hdmitx_set_drm_pkt: tf=1, cf=1, colormetry=0
[  280.105196] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  280.107304] [hdmitx:] hdmitx_set_dispmode[1551] frl_rate 0 htotal 5280 cs 1 cd 6 h_unstable 0
[  280.148638] [hdmitx:] set21_phy_by_mode_s7d[188] rterm = 7
[  280.150016] [hdmitx:] Sink is HDMI device
[  280.150169] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  280.150864] [hdmitx:] set audio
[  280.151338] [hdmitx:] audio_param->chs = 1
[  280.151986] [hdmitx:] aud_src_if = 0
[  280.152608] [hdmitx:] aud_n_para = 5120
[  280.153218] [hdmitx:] audio state: AUDIO_UNMUTE
[  280.153898] [hdmitx:] vinfo: set cur_enc_ppc as 1, vpp color: 0
[  280.154983] DOLBY: vout_notify_callback: VOUT_EVENT_MODE_CHANGE
[  280.155655] vsync_pts_inc 3600 1/25
[  280.156383] [drm] meson_vout_update_mode_name: hdmitx update vout 1 name 2160p25hz.
[  280.174517] [snd-soc]: spdif_a is set to disable
[  280.174586] [snd-soc]: aml_audio_reset, reg 0xa, shift 9, use_vadtop 0
[  280.174862] [snd-soc]: aml_audio_reset, reg 0xa, shift 14, use_vadtop 0
[  280.175856] [snd-soc]: hdmitx src switch to spdif 0
[  280.176620] [snd-soc]: sharebuffer_spdifout_prepare  get_hdmitx_audio_src(rtd->card):0  spdif_id:0
[  280.177845] [hdmitx:] hdmitx_audio_notify_callback[798] audio prepare
[  280.178770] [snd-soc]: spdif_a fifo ctrl, frddr:0 type:1, 16 bits, chmask 0x3, swap 0x10
[  280.178781] [hdmitx:] hdmitx_audio_notify_callback[803] type:1 rate:3 size:1 chs:2 i2s_ch_mask:1 aud_src_if:0
[  280.180144] [hdmitx:] aout notify format CT_PCM
[  280.180869] [hdmitx:] set audio
[  280.181386] [hdmitx:] audio_param->chs = 1
[  280.182032] [hdmitx:] aud_src_if = 0
[  280.182620] [hdmitx:] aud_n_para = 5120
[  280.183260] [hdmitx:] audio state: AUDIO_UNMUTE
[  280.183947] [hdmitx:] set audio param
[  280.184629] [snd-soc]: spdif_a is set to enable
[  280.185200] [hdmitx:] hdmitx_set_drm_pkt: tf=16, cf=9, colormetry=0
[  280.209895] [hdmitx:] avmute_store -1
[  284.435077] [hdmitx:] avmute_store 1
[  284.535379] [hdmitx:] phy_store 0
[  284.705574] [drm] [meson_encoder_vrr_change], seamless is 0
[  284.705746] [drm] build_hdmitx_attr_str:422,12bit = 1+12
[  284.706634] [drm] [meson_hdmitx_encoder_atomic_disable]
[  284.707334] [drm] am_meson_crtc_atomic_disable-[0]:in
[  284.708235] [hdmitx:] hdmitx_set_drm_pkt: disable drm pkt
[  284.709052] [hdmitx:] TV not support DV, clr dv_vsif
[  284.709724] [hdmitx:] DV H14b VSIF, switching signal to SDR
[  284.710613] [hdmitx:] hdmitx_set_hdr10plus_pkt: null vsif
[  284.711447] [hdmitx:] hdmitx_unregister_vrr ret = 0
[  284.712078] [drm] am_meson_crtc_atomic_enable-[0] in: new[2160p30hz], old[2160p25hz], vmode[4-4], uboot[0]
[  284.713476] [drm] am_meson_crtc_atomic_enable-[0]: enable mode 2160p30hz final vmode 0
[  284.714903] [hdmitx:] set21_s7d_htxpll_clk_out[96] htxpll vco 5940000 div 2
[  284.715929] [hdmitx:] pll_od0 = 1, pll_od2 = 1, pll_od1 = 2
[  284.716391] [hdmitx:] clocks_set_vid_clk_div_for_hdmi[402] div = 6
[  284.717350] [hdmitx:] configure venc
[  284.717900] [hdmitx:] config_tv_enc_calc[63] vic = 95
[  284.718661] [hdmitx:] hdmitx_soft_reset[1263]
[  284.719344] [hdmitx:]  config hdmitx IP vic = 95 cd:6 cs: 1
[  284.720159] [hdmitx:] configure hdmitx21
[  284.720816] [hdmitx:] warn: SCDC not present, should not send 1:10
[  284.722762] [hdmitx:] enable phy to dig
[  284.722814] [hdmitx:] hdmitx_set_dispmode[1551] frl_rate 0 htotal 4400 cs 1 cd 6 h_unstable 0
[  284.722882] [hdmitx:] hdmitx_set_drm_pkt: tf=1, cf=1, colormetry=0
[  284.724827] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  284.760733] [hdmitx:] set21_phy_by_mode_s7d[188] rterm = 7
[  284.762116] [hdmitx:] Sink is HDMI device
[  284.762332] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  284.762999] [hdmitx:] set audio
[  284.763440] [hdmitx:] audio_param->chs = 1
[  284.764088] [hdmitx:] aud_src_if = 0
[  284.764702] [hdmitx:] aud_n_para = 5120
[  284.765326] [hdmitx:] audio state: AUDIO_UNMUTE
[  284.765998] [hdmitx:] vinfo: set cur_enc_ppc as 1, vpp color: 0
[  284.767121] DOLBY: vout_notify_callback: VOUT_EVENT_MODE_CHANGE
[  284.767757] vsync_pts_inc 3000 1/30
[  284.768500] [drm] meson_vout_update_mode_name: hdmitx update vout 1 name 2160p30hz.
[  284.772305] [snd-soc]: spdif_a is set to disable
[  284.772388] [snd-soc]: aml_audio_reset, reg 0xa, shift 9, use_vadtop 0
[  284.772716] [snd-soc]: aml_audio_reset, reg 0xa, shift 14, use_vadtop 0
[  284.773669] [snd-soc]: hdmitx src switch to spdif 0
[  284.774376] [snd-soc]: sharebuffer_spdifout_prepare  get_hdmitx_audio_src(rtd->card):0  spdif_id:0
[  284.775651] [hdmitx:] hdmitx_audio_notify_callback[798] audio prepare
[  284.776597] [snd-soc]: spdif_a fifo ctrl, frddr:0 type:1, 16 bits, chmask 0x3, swap 0x10
[  284.776612] [hdmitx:] hdmitx_audio_notify_callback[803] type:1 rate:3 size:1 chs:2 i2s_ch_mask:1 aud_src_if:0
[  284.777952] [hdmitx:] aout notify format CT_PCM
[  284.778655] [hdmitx:] set audio
[  284.779194] [hdmitx:] audio_param->chs = 1
[  284.779839] [hdmitx:] aud_src_if = 0
[  284.780428] [hdmitx:] aud_n_para = 5120
[  284.781090] [hdmitx:] audio state: AUDIO_UNMUTE
[  284.781759] [hdmitx:] set audio param
[  284.782450] [snd-soc]: spdif_a is set to enable
[  284.789596] [hdmitx:] hdmitx_set_drm_pkt: tf=16, cf=9, colormetry=0
[  284.815628] [hdmitx:] avmute_store -1
[  289.530716] [hdmitx:] avmute_store 1
[  289.631231] [hdmitx:] phy_store 0
[  289.789891] [drm] [meson_encoder_vrr_change], seamless is 0
[  289.790067] [drm] build_hdmitx_attr_str:422,12bit = 1+12
[  289.790969] [drm] [meson_hdmitx_encoder_atomic_disable]
[  289.791655] [drm] am_meson_crtc_atomic_disable-[0]:in
[  289.792569] [hdmitx:] hdmitx_set_drm_pkt: disable drm pkt
[  289.793448] [hdmitx:] TV not support DV, clr dv_vsif
[  289.794069] [hdmitx:] DV H14b VSIF, switching signal to SDR
[  289.794968] [hdmitx:] hdmitx_set_hdr10plus_pkt: null vsif
[  289.795766] [hdmitx:] hdmitx_unregister_vrr ret = 0
[  289.796480] [drm] am_meson_crtc_atomic_enable-[0] in: new[2160p25hz], old[2160p30hz], vmode[4-4], uboot[0]
[  289.797839] [drm] am_meson_crtc_atomic_enable-[0]: enable mode 2160p25hz final vmode 0
[  289.799583] [hdmitx:] set21_s7d_htxpll_clk_out[96] htxpll vco 5940000 div 2
[  289.800284] [hdmitx:] pll_od0 = 1, pll_od2 = 1, pll_od1 = 2
[  289.800769] [hdmitx:] clocks_set_vid_clk_div_for_hdmi[402] div = 6
[  289.801682] [hdmitx:] configure venc
[  289.802240] [hdmitx:] config_tv_enc_calc[63] vic = 94
[  289.803019] [hdmitx:] hdmitx_soft_reset[1263]
[  289.803704] [hdmitx:]  config hdmitx IP vic = 94 cd:6 cs: 1
[  289.804524] [hdmitx:] configure hdmitx21
[  289.805165] [hdmitx:] warn: SCDC not present, should not send 1:10
[  289.807153] [hdmitx:] enable phy to dig
[  289.807301] [hdmitx:] hdmitx_set_drm_pkt: tf=1, cf=1, colormetry=0
[  289.807313] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  289.808892] [hdmitx:] hdmitx_set_dispmode[1551] frl_rate 0 htotal 5280 cs 1 cd 6 h_unstable 0
[  289.848689] [hdmitx:] set21_phy_by_mode_s7d[188] rterm = 7
[  289.850021] [hdmitx:] Sink is HDMI device
[  289.850158] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  289.850862] [hdmitx:] set audio
[  289.851345] [hdmitx:] audio_param->chs = 1
[  289.851992] [hdmitx:] aud_src_if = 0
[  289.852612] [hdmitx:] aud_n_para = 5120
[  289.853219] [hdmitx:] audio state: AUDIO_UNMUTE
[  289.853903] [hdmitx:] vinfo: set cur_enc_ppc as 1, vpp color: 0
[  289.854977] DOLBY: vout_notify_callback: VOUT_EVENT_MODE_CHANGE
[  289.855659] vsync_pts_inc 3600 1/25
[  289.856383] [drm] meson_vout_update_mode_name: hdmitx update vout 1 name 2160p25hz.
[  289.883551] [snd-soc]: spdif_a is set to disable
[  289.883627] [snd-soc]: aml_audio_reset, reg 0xa, shift 9, use_vadtop 0
[  289.883903] [snd-soc]: aml_audio_reset, reg 0xa, shift 14, use_vadtop 0
[  289.884917] [snd-soc]: hdmitx src switch to spdif 0
[  289.885611] [snd-soc]: sharebuffer_spdifout_prepare  get_hdmitx_audio_src(rtd->card):0  spdif_id:0
[  289.886882] [hdmitx:] hdmitx_audio_notify_callback[798] audio prepare
[  289.887294] [hdmitx:] hdmitx_set_drm_pkt: tf=16, cf=9, colormetry=0
[  289.887811] [snd-soc]: spdif_a fifo ctrl, frddr:0 type:1, 16 bits, chmask 0x3, swap 0x10
[  289.888769] [hdmitx:] hdmitx_audio_notify_callback[803] type:1 rate:3 size:1 chs:2 i2s_ch_mask:1 aud_src_if:0
[  289.890106] [hdmitx:] aout notify format CT_PCM
[  289.890811] [hdmitx:] set audio
[  289.891348] [hdmitx:] audio_param->chs = 1
[  289.891995] [hdmitx:] aud_src_if = 0
[  289.892610] [hdmitx:] aud_n_para = 5120
[  289.893229] [hdmitx:] audio state: AUDIO_UNMUTE
[  289.893916] [hdmitx:] set audio param
[  289.894602] [snd-soc]: spdif_a is set to enable
[  289.913667] [hdmitx:] avmute_store -1
[  294.936833] [hdmitx:] avmute_store 1
[  295.037155] [hdmitx:] phy_store 0
[  295.207521] [drm] [meson_encoder_vrr_change], seamless is 0
[  295.207692] [drm] build_hdmitx_attr_str:422,12bit = 1+12
[  295.208602] [drm] [meson_hdmitx_encoder_atomic_disable]
[  295.209282] [drm] am_meson_crtc_atomic_disable-[0]:in
[  295.210177] [hdmitx:] hdmitx_set_drm_pkt: disable drm pkt
[  295.210992] [hdmitx:] TV not support DV, clr dv_vsif
[  295.211683] [hdmitx:] DV H14b VSIF, switching signal to SDR
[  295.212613] [hdmitx:] hdmitx_set_hdr10plus_pkt: null vsif
[  295.213394] [hdmitx:] hdmitx_unregister_vrr ret = 0
[  295.214024] [drm] am_meson_crtc_atomic_enable-[0] in: new[2160p24hz], old[2160p25hz], vmode[4-4], uboot[0]
[  295.215388] [drm] am_meson_crtc_atomic_enable-[0]: enable mode 2160p24hz final vmode 0
[  295.216828] [hdmitx:] set21_s7d_htxpll_clk_out[96] htxpll vco 5940000 div 2
[  295.217870] [hdmitx:] pll_od0 = 1, pll_od2 = 1, pll_od1 = 2
[  295.218331] [hdmitx:] clocks_set_vid_clk_div_for_hdmi[402] div = 6
[  295.219263] [hdmitx:] configure venc
[  295.219821] [hdmitx:] config_tv_enc_calc[63] vic = 93
[  295.220624] [hdmitx:] hdmitx_soft_reset[1263]
[  295.221288] [hdmitx:]  config hdmitx IP vic = 93 cd:6 cs: 1
[  295.222105] [hdmitx:] configure hdmitx21
[  295.222735] [hdmitx:] warn: SCDC not present, should not send 1:10
[  295.224730] [hdmitx:] enable phy to dig
[  295.224780] [hdmitx:] hdmitx_set_dispmode[1551] frl_rate 0 htotal 5500 cs 1 cd 6 h_unstable 0
[  295.224860] [hdmitx:] hdmitx_set_drm_pkt: tf=1, cf=1, colormetry=0
[  295.226789] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  295.264638] [hdmitx:] set21_phy_by_mode_s7d[188] rterm = 7
[  295.265959] [hdmitx:] Sink is HDMI device
[  295.266102] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  295.266798] [hdmitx:] set audio
[  295.267273] [hdmitx:] audio_param->chs = 1
[  295.267921] [hdmitx:] aud_src_if = 0
[  295.268510] [hdmitx:] aud_n_para = 5120
[  295.269172] [hdmitx:] audio state: AUDIO_UNMUTE
[  295.269832] [hdmitx:] vinfo: set cur_enc_ppc as 1, vpp color: 0
[  295.270918] DOLBY: vout_notify_callback: VOUT_EVENT_MODE_CHANGE
[  295.271589] vsync_pts_inc 3750 1/24
[  295.272317] [drm] meson_vout_update_mode_name: hdmitx update vout 1 name 2160p24hz.
[  295.283140] [snd-soc]: spdif_a is set to disable
[  295.283226] [snd-soc]: aml_audio_reset, reg 0xa, shift 9, use_vadtop 0
[  295.283508] [snd-soc]: aml_audio_reset, reg 0xa, shift 14, use_vadtop 0
[  295.284503] [snd-soc]: hdmitx src switch to spdif 0
[  295.285246] [snd-soc]: sharebuffer_spdifout_prepare  get_hdmitx_audio_src(rtd->card):0  spdif_id:0
[  295.286492] [hdmitx:] hdmitx_audio_notify_callback[798] audio prepare
[  295.287414] [snd-soc]: spdif_a fifo ctrl, frddr:0 type:1, 16 bits, chmask 0x3, swap 0x10
[  295.287428] [hdmitx:] hdmitx_audio_notify_callback[803] type:1 rate:3 size:1 chs:2 i2s_ch_mask:1 aud_src_if:0
[  295.288808] [hdmitx:] aout notify format CT_PCM
[  295.289494] [hdmitx:] set audio
[  295.290033] [hdmitx:] audio_param->chs = 1
[  295.290677] [hdmitx:] aud_src_if = 0
[  295.291267] [hdmitx:] aud_n_para = 5120
[  295.291914] [hdmitx:] audio state: AUDIO_UNMUTE
[  295.292608] [hdmitx:] set audio param
[  295.293286] [snd-soc]: spdif_a is set to enable
[  295.308224] [hdmitx:] hdmitx_set_drm_pkt: tf=16, cf=9, colormetry=0
[  295.335306] [hdmitx:] avmute_store -1
[  301.774150] [hdmitx:] avmute_store 1
[  301.874472] [hdmitx:] phy_store 0
[  302.016791] [drm] [meson_encoder_vrr_change], seamless is 0
[  302.016962] [drm] build_hdmitx_attr_str:422,12bit = 1+12
[  302.017870] [drm] [meson_hdmitx_encoder_atomic_disable]
[  302.018554] [drm] am_meson_crtc_atomic_disable-[0]:in
[  302.019462] [hdmitx:] hdmitx_set_drm_pkt: disable drm pkt
[  302.020235] [hdmitx:] TV not support DV, clr dv_vsif
[  302.020938] [hdmitx:] DV H14b VSIF, switching signal to SDR
[  302.021865] [hdmitx:] hdmitx_set_hdr10plus_pkt: null vsif
[  302.022637] [hdmitx:] hdmitx_unregister_vrr ret = 0
[  302.023292] [drm] am_meson_crtc_atomic_enable-[0] in: new[2160p30hz], old[2160p24hz], vmode[4-4], uboot[0]
[  302.024851] [drm] am_meson_crtc_atomic_enable-[0]: enable mode 2160p30hz final vmode 0
[  302.026086] [hdmitx:] set21_s7d_htxpll_clk_out[96] htxpll vco 5940000 div 2
[  302.027169] [hdmitx:] pll_od0 = 1, pll_od2 = 1, pll_od1 = 2
[  302.027601] [hdmitx:] clocks_set_vid_clk_div_for_hdmi[402] div = 6
[  302.028604] [hdmitx:] configure venc
[  302.029094] [hdmitx:] config_tv_enc_calc[63] vic = 95
[  302.029875] [hdmitx:] hdmitx_soft_reset[1263]
[  302.030561] [hdmitx:]  config hdmitx IP vic = 95 cd:6 cs: 1
[  302.031376] [hdmitx:] configure hdmitx21
[  302.032005] [hdmitx:] warn: SCDC not present, should not send 1:10
[  302.034015] [hdmitx:] enable phy to dig
[  302.034147] [hdmitx:] hdmitx_set_drm_pkt: tf=1, cf=1, colormetry=0
[  302.034166] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  302.036855] [hdmitx:] hdmitx_set_dispmode[1551] frl_rate 0 htotal 4400 cs 1 cd 6 h_unstable 0
[  302.076634] [hdmitx:] set21_phy_by_mode_s7d[188] rterm = 7
[  302.077995] [hdmitx:] Sink is HDMI device
[  302.078198] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  302.078868] [hdmitx:] set audio
[  302.079311] [hdmitx:] audio_param->chs = 1
[  302.079959] [hdmitx:] aud_src_if = 0
[  302.080549] [hdmitx:] aud_n_para = 5120
[  302.081236] [hdmitx:] audio state: AUDIO_UNMUTE
[  302.081867] [hdmitx:] vinfo: set cur_enc_ppc as 1, vpp color: 0
[  302.082984] DOLBY: vout_notify_callback: VOUT_EVENT_MODE_CHANGE
[  302.083625] vsync_pts_inc 3000 1/30
[  302.084354] [drm] meson_vout_update_mode_name: hdmitx update vout 1 name 2160p30hz.
[  302.089289] [snd-soc]: spdif_a is set to disable
[  302.089364] [snd-soc]: aml_audio_reset, reg 0xa, shift 9, use_vadtop 0
[  302.089645] [snd-soc]: aml_audio_reset, reg 0xa, shift 14, use_vadtop 0
[  302.090641] [snd-soc]: hdmitx src switch to spdif 0
[  302.091352] [snd-soc]: sharebuffer_spdifout_prepare  get_hdmitx_audio_src(rtd->card):0  spdif_id:0
[  302.092650] [hdmitx:] hdmitx_audio_notify_callback[798] audio prepare
[  302.093553] [snd-soc]: spdif_a fifo ctrl, frddr:0 type:1, 16 bits, chmask 0x3, swap 0x10
[  302.093567] [hdmitx:] hdmitx_audio_notify_callback[803] type:1 rate:3 size:1 chs:2 i2s_ch_mask:1 aud_src_if:0
[  302.094925] [hdmitx:] aout notify format CT_PCM
[  302.095629] [hdmitx:] set audio
[  302.096166] [hdmitx:] audio_param->chs = 1
[  302.096834] [hdmitx:] aud_src_if = 0
[  302.097403] [hdmitx:] aud_n_para = 5120
[  302.098039] [hdmitx:] audio state: AUDIO_UNMUTE
[  302.098733] [hdmitx:] set audio param
[  302.099414] [snd-soc]: spdif_a is set to enable
[  302.100816] [hdmitx:] hdmitx_set_drm_pkt: tf=16, cf=9, colormetry=0
[  302.126229] [hdmitx:] avmute_store -1
[  317.964663] type=1400 audit(1753189635.183:1165): avc:  denied  { getopt } for  comm=73657276657220736F636B6574 laddr=::ffff:192.168.0.108 lport=5555 faddr=::ffff:192.168.0.106 fport=59276 scontext=u:r:su:s0 tcontext=u:r:su:s0 tclass=tcp_socket permissive=1
[  317.965405] audit: audit_lost=268 audit_rate_limit=5 audit_backlog_limit=64
[  317.967811] type=1400 audit(1753189635.183:1166): avc:  denied  { write } for  comm=73657276657220736F636B6574 name="fwmarkd" dev="tmpfs" ino=861 scontext=u:r:su:s0 tcontext=u:object_r:fwmarkd_socket:s0 tclass=sock_file permissive=1
[  317.969073] audit: rate limit exceeded
[  317.971391] type=1400 audit(1753189635.187:1167): avc:  denied  { connectto } for  comm=73657276657220736F636B6574 path="/dev/socket/fwmarkd" scontext=u:r:su:s0 tcontext=u:r:netd:s0 tclass=unix_stream_socket permissive=1
[  317.974129] type=1400 audit(1753189635.187:1168): avc:  denied  { use } for  comm="binder:458_2" path="socket:[34862]" dev="sockfs" ino=34862 scontext=u:r:netd:s0 tcontext=u:r:su:s0 tclass=fd permissive=1
[  317.976940] type=1400 audit(1753189635.187:1169): avc:  denied  { read write } for  comm="binder:458_2" path="socket:[34862]" dev="sockfs" ino=34862 scontext=u:r:netd:s0 tcontext=u:r:su:s0 tclass=tcp_socket permissive=1
[  317.979018] type=1400 audit(1753189635.187:1170): avc:  denied  { getopt } for  comm="binder:458_2" laddr=::ffff:192.168.0.108 lport=5555 faddr=::ffff:192.168.0.106 fport=59276 scontext=u:r:netd:s0 tcontext=u:r:su:s0 tclass=tcp_socket permissive=1
[  317.982016] type=1400 audit(1753189635.187:1171): avc:  denied  { setopt } for  comm="binder:458_2" laddr=::ffff:192.168.0.108 lport=5555 faddr=::ffff:192.168.0.106 fport=59276 scontext=u:r:netd:s0 tcontext=u:r:su:s0 tclass=tcp_socket permissive=1
[  317.984760] type=1400 audit(1753189635.187:1172): avc:  denied  { setopt } for  comm=73657276657220736F636B6574 laddr=::ffff:192.168.0.108 lport=5555 faddr=::ffff:192.168.0.106 fport=59276 scontext=u:r:su:s0 tcontext=u:r:su:s0 tclass=tcp_socket permissive=1
[  320.471759] type=1400 audit(1753189637.691:1180): avc:  denied  { read } for  comm="adbd" name="u:object_r:device_logging_prop:s0" dev="tmpfs" ino=213 scontext=u:r:su:s0 tcontext=u:object_r:device_logging_prop:s0 tclass=file permissive=1
[  320.474122] type=1400 audit(1753189637.691:1181): avc:  denied  { open } for  comm="adbd" path="/dev/__properties__/u:object_r:device_logging_prop:s0" dev="tmpfs" ino=213 scontext=u:r:su:s0 tcontext=u:object_r:device_logging_prop:s0 tclass=file permissive=1
[  320.475114] audit: audit_lost=275 audit_rate_limit=5 audit_backlog_limit=64
[  320.477873] audit: rate limit exceeded
[  324.588628] [aml_send_sync_trace 4388] sync token[36943]
[  324.588651] >>> aml_send_msg()
[  324.589572] ipc_sdio_host_msgack_handler 000000002aa4e30a
[  324.590107] [aml_msgackind 2039] msg ack hostid=0xffffff8000885e80
[  324.591015] [cmd_mgr_llind         329] cmd tkn[42]  flags:0008  result: -4  cmd: 105-MM_SYNC_TRACE            - reqcfm(   0-none)
[  324.592641] [cmd_complete           65] cmd tkn[42]  flags:0000  result: -4  cmd: 105-MM_SYNC_TRACE            - reqcfm(   0-none)
[  325.371421] type=1400 audit(1753189642.591:1201): avc:  denied  { read } for  comm="cling--ap-1" name="address" dev="sysfs" ino=22143 scontext=u:r:untrusted_app_27:s0:c43,c256,c512,c768 tcontext=u:object_r:sysfs_net:s0 tclass=file permissive=1 app=com.dangbei.screencast
[  325.374092] type=1400 audit(1753189642.591:1202): avc:  denied  { open } for  comm="cling--ap-1" path="/sys/devices/virtual/net/dummy0/address" dev="sysfs" ino=22143 scontext=u:r:untrusted_app_27:s0:c43,c256,c512,c768 tcontext=u:object_r:sysfs_net:s0 tclass=file permissive=1 app=com.dangbei.screencast
[  325.377517] type=1400 audit(1753189642.591:1203): avc:  denied  { getattr } for  comm="cling--ap-1" path="/sys/devices/virtual/net/dummy0/address" dev="sysfs" ino=22143 scontext=u:r:untrusted_app_27:s0:c43,c256,c512,c768 tcontext=u:object_r:sysfs_net:s0 tclass=file permissive=1 app=com.dangbei.screencast
[  336.057153] [SP FRAME RX] arp req,vif_idx:0 sender:[f8:8c:21:8f:40:25 192.168.0.1]receiver:[00:00:00:00:00:00 192.168.0.108]
[  336.058114] [SP FRAME TX] arp rsp,vif_idx:0 sender:[c0:e3:50:49:af:ae 192.168.0.108]receiver:[f8:8c:21:8f:40:25 192.168.0.1]
[  344.369270] type=1400 audit(1753189661.591:1204): avc:  denied  { getattr } for  comm="sh" path="/system/bin/logcat" dev="dm-8" ino=27552265 scontext=u:r:su:s0 tcontext=u:object_r:logcat_exec:s0 tclass=file permissive=1
[  344.371867] type=1400 audit(1753189661.591:1205): avc:  denied  { execute } for  comm="sh" name="logcat" dev="dm-8" ino=27552265 scontext=u:r:su:s0 tcontext=u:object_r:logcat_exec:s0 tclass=file permissive=1
[  344.374981] type=1400 audit(1753189661.591:1206): avc:  denied  { read open } for  comm="sh" path="/system/bin/logcat" dev="dm-8" ino=27552265 scontext=u:r:su:s0 tcontext=u:object_r:logcat_exec:s0 tclass=file permissive=1
[  344.377272] type=1400 audit(1753189661.591:1207): avc:  denied  { execute_no_trans } for  comm="sh" path="/system/bin/logcat" dev="dm-8" ino=27552265 scontext=u:r:su:s0 tcontext=u:object_r:logcat_exec:s0 tclass=file permissive=1
[  344.381383] type=1400 audit(1753189661.603:1208): avc:  denied  { map } for  comm="logcat" path="/system/bin/logcat" dev="dm-8" ino=27552265 scontext=u:r:su:s0 tcontext=u:object_r:logcat_exec:s0 tclass=file permissive=1
[  344.384265] type=1400 audit(1753189661.603:1209): avc:  denied  { getattr } for  comm="logcat" path="/system/bin/logcat" dev="dm-8" ino=27552265 scontext=u:r:su:s0 tcontext=u:object_r:logcat_exec:s0 tclass=file permissive=1
[  344.398366] type=1400 audit(1753189661.619:1210): avc:  denied  { read } for  comm="logcat" path="/system/bin/logcat" dev="dm-8" ino=27552265 scontext=u:r:su:s0 tcontext=u:object_r:logcat_exec:s0 tclass=file permissive=1
[  344.403746] audit: audit_lost=287 audit_rate_limit=5 audit_backlog_limit=64
[  344.403859] type=1400 audit(1753189661.623:1211): avc:  denied  { write } for  comm="logcat" name="logd" dev="tmpfs" ino=750 scontext=u:r:su:s0 tcontext=u:object_r:logd_socket:s0 tclass=sock_file permissive=1
[  344.404098] audit: rate limit exceeded
[  347.693223] type=1400 audit(1753189664.915:1213): avc:  denied  { read write } for  comm=75736220666673206F70656E name="ep0" dev="functionfs" ino=25199 scontext=u:r:su:s0 tcontext=u:object_r:functionfs:s0 tclass=file permissive=1
[  347.695506] type=1400 audit(1753189664.915:1214): avc:  denied  { open } for  comm=75736220666673206F70656E path="/dev/usb-ffs/adb/ep0" dev="functionfs" ino=25199 scontext=u:r:su:s0 tcontext=u:object_r:functionfs:s0 tclass=file permissive=1
[  347.776210] [hdmitx:] avmute_store 1
[  347.876497] [hdmitx:] phy_store 0
[  348.034518] [drm] [meson_encoder_vrr_change], seamless is 0
[  348.034694] [drm] build_hdmitx_attr_str:422,12bit = 1+12
[  348.035599] [drm] [meson_hdmitx_encoder_atomic_disable]
[  348.036282] [drm] am_meson_crtc_atomic_disable-[0]:in
[  348.037233] [hdmitx:] hdmitx_set_drm_pkt: disable drm pkt
[  348.037993] [hdmitx:] TV not support DV, clr dv_vsif
[  348.038683] [hdmitx:] DV H14b VSIF, switching signal to SDR
[  348.039593] [hdmitx:] hdmitx_set_hdr10plus_pkt: null vsif
[  348.040392] [hdmitx:] hdmitx_unregister_vrr ret = 0
[  348.041049] [drm] am_meson_crtc_atomic_enable-[0] in: new[2160p25hz], old[2160p30hz], vmode[4-4], uboot[0]
[  348.042387] [drm] am_meson_crtc_atomic_enable-[0]: enable mode 2160p25hz final vmode 0
[  348.043807] [hdmitx:] set21_s7d_htxpll_clk_out[96] htxpll vco 5940000 div 2
[  348.044839] [hdmitx:] pll_od0 = 1, pll_od2 = 1, pll_od1 = 2
[  348.045331] [hdmitx:] clocks_set_vid_clk_div_for_hdmi[402] div = 6
[  348.046260] [hdmitx:] configure venc
[  348.046821] [hdmitx:] config_tv_enc_calc[63] vic = 94
[  348.047600] [hdmitx:] hdmitx_soft_reset[1263]
[  348.048285] [hdmitx:]  config hdmitx IP vic = 94 cd:6 cs: 1
[  348.049121] [hdmitx:] configure hdmitx21
[  348.049740] [hdmitx:] warn: SCDC not present, should not send 1:10
[  348.051715] [hdmitx:] enable phy to dig
[  348.051766] [hdmitx:] hdmitx_set_dispmode[1551] frl_rate 0 htotal 5280 cs 1 cd 6 h_unstable 0
[  348.051845] [hdmitx:] hdmitx_set_drm_pkt: tf=1, cf=1, colormetry=0
[  348.053777] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  348.092643] [hdmitx:] set21_phy_by_mode_s7d[188] rterm = 7
[  348.093978] [hdmitx:] Sink is HDMI device
[  348.094141] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  348.094873] [hdmitx:] set audio
[  348.095293] [hdmitx:] audio_param->chs = 1
[  348.095939] [hdmitx:] aud_src_if = 0
[  348.096528] [hdmitx:] aud_n_para = 5120
[  348.097208] [hdmitx:] audio state: AUDIO_UNMUTE
[  348.097850] [hdmitx:] vinfo: set cur_enc_ppc as 1, vpp color: 0
[  348.098966] DOLBY: vout_notify_callback: VOUT_EVENT_MODE_CHANGE
[  348.099609] vsync_pts_inc 3600 1/25
[  348.100371] [drm] meson_vout_update_mode_name: hdmitx update vout 1 name 2160p25hz.
[  348.127585] [snd-soc]: spdif_a is set to disable
[  348.127656] [snd-soc]: aml_audio_reset, reg 0xa, shift 9, use_vadtop 0
[  348.127931] [snd-soc]: aml_audio_reset, reg 0xa, shift 14, use_vadtop 0
[  348.128950] [snd-soc]: hdmitx src switch to spdif 0
[  348.129638] [snd-soc]: sharebuffer_spdifout_prepare  get_hdmitx_audio_src(rtd->card):0  spdif_id:0
[  348.130910] [hdmitx:] hdmitx_audio_notify_callback[798] audio prepare
[  348.131837] [snd-soc]: spdif_a fifo ctrl, frddr:0 type:1, 16 bits, chmask 0x3, swap 0x10
[  348.131840] [hdmitx:] hdmitx_set_drm_pkt: tf=16, cf=9, colormetry=0
[  348.131847] [hdmitx:] hdmitx_audio_notify_callback[803] type:1 rate:3 size:1 chs:2 i2s_ch_mask:1 aud_src_if:0
[  348.134134] [hdmitx:] aout notify format CT_PCM
[  348.134839] [hdmitx:] set audio
[  348.135375] [hdmitx:] audio_param->chs = 1
[  348.136022] [hdmitx:] aud_src_if = 0
[  348.136622] [hdmitx:] aud_n_para = 5120
[  348.137252] [hdmitx:] audio state: AUDIO_UNMUTE
[  348.137937] [hdmitx:] set audio param
[  348.138622] [snd-soc]: spdif_a is set to enable
[  348.158716] [hdmitx:] avmute_store -1
[  352.180978] [hdmitx:] avmute_store 1
[  352.281269] [hdmitx:] phy_store 0
[  352.452116] [drm] [meson_encoder_vrr_change], seamless is 0
[  352.452289] [drm] build_hdmitx_attr_str:422,12bit = 1+12
[  352.453225] [drm] [meson_hdmitx_encoder_atomic_disable]
[  352.453878] [drm] am_meson_crtc_atomic_disable-[0]:in
[  352.454854] [hdmitx:] hdmitx_set_drm_pkt: disable drm pkt
[  352.455589] [hdmitx:] TV not support DV, clr dv_vsif
[  352.456278] [hdmitx:] DV H14b VSIF, switching signal to SDR
[  352.457217] [hdmitx:] hdmitx_set_hdr10plus_pkt: null vsif
[  352.458007] [hdmitx:] hdmitx_unregister_vrr ret = 0
[  352.458621] [drm] am_meson_crtc_atomic_enable-[0] in: new[2160p30hz], old[2160p25hz], vmode[4-4], uboot[0]
[  352.459987] [drm] am_meson_crtc_atomic_enable-[0]: enable mode 2160p30hz final vmode 0
[  352.461451] [hdmitx:] set21_s7d_htxpll_clk_out[96] htxpll vco 5940000 div 2
[  352.462502] [hdmitx:] pll_od0 = 1, pll_od2 = 1, pll_od1 = 2
[  352.462926] [hdmitx:] clocks_set_vid_clk_div_for_hdmi[402] div = 6
[  352.464124] [hdmitx:] configure venc
[  352.464418] [hdmitx:] config_tv_enc_calc[63] vic = 95
[  352.465217] [hdmitx:] hdmitx_soft_reset[1263]
[  352.465881] [hdmitx:]  config hdmitx IP vic = 95 cd:6 cs: 1
[  352.466700] [hdmitx:] configure hdmitx21
[  352.467330] [hdmitx:] warn: SCDC not present, should not send 1:10
[  352.469297] [hdmitx:] enable phy to dig
[  352.469422] [hdmitx:] hdmitx_set_drm_pkt: tf=1, cf=1, colormetry=0
[  352.470282] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  352.471599] [hdmitx:] hdmitx_set_dispmode[1551] frl_rate 0 htotal 4400 cs 1 cd 6 h_unstable 0
[  352.508661] [hdmitx:] set21_phy_by_mode_s7d[188] rterm = 7
[  352.509972] [hdmitx:] Sink is HDMI device
[  352.510096] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  352.510798] [hdmitx:] set audio
[  352.511279] [hdmitx:] audio_param->chs = 1
[  352.511927] [hdmitx:] aud_src_if = 0
[  352.512516] [hdmitx:] aud_n_para = 5120
[  352.513179] [hdmitx:] audio state: AUDIO_UNMUTE
[  352.513836] [hdmitx:] vinfo: set cur_enc_ppc as 1, vpp color: 0
[  352.514913] DOLBY: vout_notify_callback: VOUT_EVENT_MODE_CHANGE
[  352.515595] vsync_pts_inc 3000 1/30
[  352.516258] [drm] meson_vout_update_mode_name: hdmitx update vout 1 name 2160p30hz.
[  352.535528] [snd-soc]: spdif_a is set to disable
[  352.535604] [snd-soc]: aml_audio_reset, reg 0xa, shift 9, use_vadtop 0
[  352.535880] [snd-soc]: aml_audio_reset, reg 0xa, shift 14, use_vadtop 0
[  352.536108] [hdmitx:] hdmitx_set_drm_pkt: tf=16, cf=9, colormetry=0
[  352.536905] [snd-soc]: hdmitx src switch to spdif 0
[  352.538508] [snd-soc]: sharebuffer_spdifout_prepare  get_hdmitx_audio_src(rtd->card):0  spdif_id:0
[  352.539779] [hdmitx:] hdmitx_audio_notify_callback[798] audio prepare
[  352.540823] [snd-soc]: spdif_a fifo ctrl, frddr:0 type:1, 16 bits, chmask 0x3, swap 0x10
[  352.540847] [hdmitx:] hdmitx_audio_notify_callback[803] type:1 rate:3 size:1 chs:2 i2s_ch_mask:1 aud_src_if:0
[  352.542087] [hdmitx:] aout notify format CT_PCM
[  352.542787] [hdmitx:] set audio
[  352.543330] [hdmitx:] audio_param->chs = 1
[  352.543972] [hdmitx:] aud_src_if = 0
[  352.544561] [hdmitx:] aud_n_para = 5120
[  352.545308] [hdmitx:] audio state: AUDIO_UNMUTE
[  352.545891] [hdmitx:] set audio param
[  352.546581] [snd-soc]: spdif_a is set to enable
[  352.564147] [hdmitx:] avmute_store -1
[  356.810701] [hdmitx:] avmute_store 1
[  356.911023] [hdmitx:] phy_store 0
[  357.069689] [drm] [meson_encoder_vrr_change], seamless is 0
[  357.069865] [drm] build_hdmitx_attr_str:422,12bit = 1+12
[  357.070761] [drm] [meson_hdmitx_encoder_atomic_disable]
[  357.071453] [drm] am_meson_crtc_atomic_disable-[0]:in
[  357.072361] [hdmitx:] hdmitx_set_drm_pkt: disable drm pkt
[  357.073180] [hdmitx:] TV not support DV, clr dv_vsif
[  357.073848] [hdmitx:] DV H14b VSIF, switching signal to SDR
[  357.074732] [hdmitx:] hdmitx_set_hdr10plus_pkt: null vsif
[  357.075547] [hdmitx:] hdmitx_unregister_vrr ret = 0
[  357.076195] [drm] am_meson_crtc_atomic_enable-[0] in: new[2160p25hz], old[2160p30hz], vmode[4-4], uboot[0]
[  357.077580] [drm] am_meson_crtc_atomic_enable-[0]: enable mode 2160p25hz final vmode 0
[  357.079001] [hdmitx:] set21_s7d_htxpll_clk_out[96] htxpll vco 5940000 div 2
[  357.080044] [hdmitx:] pll_od0 = 1, pll_od2 = 1, pll_od1 = 2
[  357.080502] [hdmitx:] clocks_set_vid_clk_div_for_hdmi[402] div = 6
[  357.081470] [hdmitx:] configure venc
[  357.081993] [hdmitx:] config_tv_enc_calc[63] vic = 94
[  357.082775] [hdmitx:] hdmitx_soft_reset[1263]
[  357.083461] [hdmitx:]  config hdmitx IP vic = 94 cd:6 cs: 1
[  357.084277] [hdmitx:] configure hdmitx21
[  357.084924] [hdmitx:] warn: SCDC not present, should not send 1:10
[  357.086898] [hdmitx:] enable phy to dig
[  357.086951] [hdmitx:] hdmitx_set_dispmode[1551] frl_rate 0 htotal 5280 cs 1 cd 6 h_unstable 0
[  357.087031] [hdmitx:] hdmitx_set_drm_pkt: tf=1, cf=1, colormetry=0
[  357.088967] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  357.124629] [hdmitx:] set21_phy_by_mode_s7d[188] rterm = 7
[  357.125991] [hdmitx:] Sink is HDMI device
[  357.126193] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  357.126863] [hdmitx:] set audio
[  357.127305] [hdmitx:] audio_param->chs = 1
[  357.127953] [hdmitx:] aud_src_if = 0
[  357.128543] [hdmitx:] aud_n_para = 5120
[  357.129231] [hdmitx:] audio state: AUDIO_UNMUTE
[  357.129863] [hdmitx:] vinfo: set cur_enc_ppc as 1, vpp color: 0
[  357.130991] DOLBY: vout_notify_callback: VOUT_EVENT_MODE_CHANGE
[  357.131619] vsync_pts_inc 3600 1/25
[  357.132347] [drm] meson_vout_update_mode_name: hdmitx update vout 1 name 2160p25hz.
[  357.133129] [snd-soc]: spdif_a is set to disable
[  357.133338] [snd-soc]: aml_audio_reset, reg 0xa, shift 9, use_vadtop 0
[  357.134240] [snd-soc]: aml_audio_reset, reg 0xa, shift 14, use_vadtop 0
[  357.135236] [snd-soc]: hdmitx src switch to spdif 0
[  357.136006] [snd-soc]: sharebuffer_spdifout_prepare  get_hdmitx_audio_src(rtd->card):0  spdif_id:0
[  357.137273] [hdmitx:] hdmitx_audio_notify_callback[798] audio prepare
[  357.138147] [snd-soc]: spdif_a fifo ctrl, frddr:0 type:1, 16 bits, chmask 0x3, swap 0x10
[  357.138161] [hdmitx:] hdmitx_audio_notify_callback[803] type:1 rate:3 size:1 chs:2 i2s_ch_mask:1 aud_src_if:0
[  357.139519] [hdmitx:] aout notify format CT_PCM
[  357.140223] [hdmitx:] set audio
[  357.140776] [hdmitx:] audio_param->chs = 1
[  357.141408] [hdmitx:] aud_src_if = 0
[  357.141997] [hdmitx:] aud_n_para = 5120
[  357.142645] [hdmitx:] audio state: AUDIO_UNMUTE
[  357.143329] [hdmitx:] set audio param
[  357.144028] [snd-soc]: spdif_a is set to enable
[  357.167034] [hdmitx:] hdmitx_set_drm_pkt: tf=16, cf=9, colormetry=0
[  357.192077] [hdmitx:] avmute_store -1
[  361.374102] [hdmitx:] avmute_store 1
[  361.474344] [hdmitx:] phy_store 0
[  361.647595] [drm] [meson_encoder_vrr_change], seamless is 0
[  361.647767] [drm] build_hdmitx_attr_str:422,12bit = 1+12
[  361.648689] [drm] [meson_hdmitx_encoder_atomic_disable]
[  361.649357] [drm] am_meson_crtc_atomic_disable-[0]:in
[  361.650240] [hdmitx:] hdmitx_set_drm_pkt: disable drm pkt
[  361.651053] [hdmitx:] TV not support DV, clr dv_vsif
[  361.651743] [hdmitx:] DV H14b VSIF, switching signal to SDR
[  361.652649] [hdmitx:] hdmitx_set_hdr10plus_pkt: null vsif
[  361.653440] [hdmitx:] hdmitx_unregister_vrr ret = 0
[  361.654097] [drm] am_meson_crtc_atomic_enable-[0] in: new[2160p30hz], old[2160p25hz], vmode[4-4], uboot[0]
[  361.655458] [drm] am_meson_crtc_atomic_enable-[0]: enable mode 2160p30hz final vmode 0
[  361.656862] [hdmitx:] set21_s7d_htxpll_clk_out[96] htxpll vco 5940000 div 2
[  361.657941] [hdmitx:] pll_od0 = 1, pll_od2 = 1, pll_od1 = 2
[  361.658407] [hdmitx:] clocks_set_vid_clk_div_for_hdmi[402] div = 6
[  361.659339] [hdmitx:] configure venc
[  361.659895] [hdmitx:] config_tv_enc_calc[63] vic = 95
[  361.660709] [hdmitx:] hdmitx_soft_reset[1263]
[  361.661365] [hdmitx:]  config hdmitx IP vic = 95 cd:6 cs: 1
[  361.662179] [hdmitx:] configure hdmitx21
[  361.662809] [hdmitx:] warn: SCDC not present, should not send 1:10
[  361.664797] [hdmitx:] enable phy to dig
[  361.664856] [hdmitx:] hdmitx_set_dispmode[1551] frl_rate 0 htotal 4400 cs 1 cd 6 h_unstable 0
[  361.664932] [hdmitx:] hdmitx_set_drm_pkt: tf=1, cf=1, colormetry=0
[  361.666868] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  361.704639] [hdmitx:] set21_phy_by_mode_s7d[188] rterm = 7
[  361.705977] [hdmitx:] Sink is HDMI device
[  361.706142] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  361.706828] [hdmitx:] set audio
[  361.707290] [hdmitx:] audio_param->chs = 1
[  361.708025] [hdmitx:] aud_src_if = 0
[  361.708533] [hdmitx:] aud_n_para = 5120
[  361.709210] [hdmitx:] audio state: AUDIO_UNMUTE
[  361.709850] [hdmitx:] vinfo: set cur_enc_ppc as 1, vpp color: 0
[  361.711003] DOLBY: vout_notify_callback: VOUT_EVENT_MODE_CHANGE
[  361.711607] vsync_pts_inc 3000 1/30
[  361.712378] [drm] meson_vout_update_mode_name: hdmitx update vout 1 name 2160p30hz.
[  361.730724] [snd-soc]: spdif_a is set to disable
[  361.730824] [snd-soc]: aml_audio_reset, reg 0xa, shift 9, use_vadtop 0
[  361.731110] [snd-soc]: aml_audio_reset, reg 0xa, shift 14, use_vadtop 0
[  361.731639] [hdmitx:] hdmitx_set_drm_pkt: tf=16, cf=9, colormetry=0
[  361.732106] [snd-soc]: hdmitx src switch to spdif 0
[  361.733740] [snd-soc]: sharebuffer_spdifout_prepare  get_hdmitx_audio_src(rtd->card):0  spdif_id:0
[  361.735011] [hdmitx:] hdmitx_audio_notify_callback[798] audio prepare
[  361.735941] [snd-soc]: spdif_a fifo ctrl, frddr:0 type:1, 16 bits, chmask 0x3, swap 0x10
[  361.735959] [hdmitx:] hdmitx_audio_notify_callback[803] type:1 rate:3 size:1 chs:2 i2s_ch_mask:1 aud_src_if:0
[  361.737360] [hdmitx:] aout notify format CT_PCM
[  361.738019] [hdmitx:] set audio
[  361.738558] [hdmitx:] audio_param->chs = 1
[  361.739202] [hdmitx:] aud_src_if = 0
[  361.739792] [hdmitx:] aud_n_para = 5120
[  361.740427] [hdmitx:] audio state: AUDIO_UNMUTE
[  361.741127] [hdmitx:] set audio param
[  361.741803] [snd-soc]: spdif_a is set to enable
[  361.760077] [hdmitx:] avmute_store -1
[  367.705397] [hdmitx:] avmute_store 1
[  367.805715] [hdmitx:] phy_store 0
[  367.965154] [drm] [meson_encoder_vrr_change], seamless is 0
[  367.965326] [drm] build_hdmitx_attr_str:422,12bit = 1+12
[  367.966215] [drm] [meson_hdmitx_encoder_atomic_disable]
[  367.966917] [drm] am_meson_crtc_atomic_disable-[0]:in
[  367.967833] [hdmitx:] hdmitx_set_drm_pkt: disable drm pkt
[  367.968622] [hdmitx:] TV not support DV, clr dv_vsif
[  367.969303] [hdmitx:] DV H14b VSIF, switching signal to SDR
[  367.970222] [hdmitx:] hdmitx_set_hdr10plus_pkt: null vsif
[  367.971276] [hdmitx:] hdmitx_unregister_vrr ret = 0
[  367.971668] [drm] am_meson_crtc_atomic_enable-[0] in: new[2160p25hz], old[2160p30hz], vmode[4-4], uboot[0]
[  367.973064] [drm] am_meson_crtc_atomic_enable-[0]: enable mode 2160p25hz final vmode 0
[  367.974439] [hdmitx:] set21_s7d_htxpll_clk_out[96] htxpll vco 5940000 div 2
[  367.975495] [hdmitx:] pll_od0 = 1, pll_od2 = 1, pll_od1 = 2
[  367.975965] [hdmitx:] clocks_set_vid_clk_div_for_hdmi[402] div = 6
[  367.976930] [hdmitx:] configure venc
[  367.977457] [hdmitx:] config_tv_enc_calc[63] vic = 94
[  367.978266] [hdmitx:] hdmitx_soft_reset[1263]
[  367.978926] [hdmitx:]  config hdmitx IP vic = 94 cd:6 cs: 1
[  367.979743] [hdmitx:] configure hdmitx21
[  367.980370] [hdmitx:] warn: SCDC not present, should not send 1:10
[  367.982381] [hdmitx:] enable phy to dig
[  367.982425] [hdmitx:] hdmitx_set_dispmode[1551] frl_rate 0 htotal 5280 cs 1 cd 6 h_unstable 0
[  367.982500] [hdmitx:] hdmitx_set_drm_pkt: tf=1, cf=1, colormetry=0
[  367.984440] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  368.020630] [hdmitx:] set21_phy_by_mode_s7d[188] rterm = 7
[  368.021949] [hdmitx:] Sink is HDMI device
[  368.022088] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  368.022785] [hdmitx:] set audio
[  368.023262] [hdmitx:] audio_param->chs = 1
[  368.023910] [hdmitx:] aud_src_if = 0
[  368.024500] [hdmitx:] aud_n_para = 5120
[  368.025184] [hdmitx:] audio state: AUDIO_UNMUTE
[  368.025820] [hdmitx:] vinfo: set cur_enc_ppc as 1, vpp color: 0
[  368.026983] DOLBY: vout_notify_callback: VOUT_EVENT_MODE_CHANGE
[  368.027578] vsync_pts_inc 3600 1/25
[  368.028356] [drm] meson_vout_update_mode_name: hdmitx update vout 1 name 2160p25hz.
[  368.057149] [snd-soc]: spdif_a is set to disable
[  368.057243] [snd-soc]: aml_audio_reset, reg 0xa, shift 9, use_vadtop 0
[  368.057527] [snd-soc]: aml_audio_reset, reg 0xa, shift 14, use_vadtop 0
[  368.058520] [snd-soc]: hdmitx src switch to spdif 0
[  368.059250] [snd-soc]: sharebuffer_spdifout_prepare  get_hdmitx_audio_src(rtd->card):0  spdif_id:0
[  368.060509] [hdmitx:] hdmitx_audio_notify_callback[798] audio prepare
[  368.061453] [snd-soc]: spdif_a fifo ctrl, frddr:0 type:1, 16 bits, chmask 0x3, swap 0x10
[  368.061470] [hdmitx:] hdmitx_audio_notify_callback[803] type:1 rate:3 size:1 chs:2 i2s_ch_mask:1 aud_src_if:0
[  368.062547] [hdmitx:] hdmitx_set_drm_pkt: tf=16, cf=9, colormetry=0
[  368.062808] [hdmitx:] aout notify format CT_PCM
[  368.062814] [hdmitx:] set audio
[  368.065009] [hdmitx:] audio_param->chs = 1
[  368.065619] [hdmitx:] aud_src_if = 0
[  368.066268] [hdmitx:] aud_n_para = 5120
[  368.066912] [hdmitx:] audio state: AUDIO_UNMUTE
[  368.067539] [hdmitx:] set audio param
[  368.068241] [snd-soc]: spdif_a is set to enable
[  368.091233] [hdmitx:] avmute_store -1
[  370.920779] [SP FRAME TX] arp req,vif_idx:0 sender:[c0:e3:50:49:af:ae 192.168.0.108]receiver:[00:00:00:00:00:00 192.168.0.106]
[  370.966662] [SP FRAME RX] arp rsp,vif_idx:0 sender:[1c:70:c9:d7:7a:54 192.168.0.106]receiver:[c0:e3:50:49:af:ae 192.168.0.108]
[  371.948349] [hdmitx:] avmute_store 1
[  372.048697] [hdmitx:] phy_store 0
[  372.222767] [drm] [meson_encoder_vrr_change], seamless is 0
[  372.222939] [drm] build_hdmitx_attr_str:422,12bit = 1+12
[  372.223832] [drm] [meson_hdmitx_encoder_atomic_disable]
[  372.224529] [drm] am_meson_crtc_atomic_disable-[0]:in
[  372.225658] [hdmitx:] hdmitx_set_drm_pkt: disable drm pkt
[  372.226242] [hdmitx:] TV not support DV, clr dv_vsif
[  372.226929] [hdmitx:] DV H14b VSIF, switching signal to SDR
[  372.227823] [hdmitx:] hdmitx_set_hdr10plus_pkt: null vsif
[  372.228848] [hdmitx:] hdmitx_unregister_vrr ret = 0
[  372.229281] [drm] am_meson_crtc_atomic_enable-[0] in: new[2160p30hz], old[2160p25hz], vmode[4-4], uboot[0]
[  372.230645] [drm] am_meson_crtc_atomic_enable-[0]: enable mode 2160p30hz final vmode 0
[  372.232061] [hdmitx:] set21_s7d_htxpll_clk_out[96] htxpll vco 5940000 div 2
[  372.233136] [hdmitx:] pll_od0 = 1, pll_od2 = 1, pll_od1 = 2
[  372.233578] [hdmitx:] clocks_set_vid_clk_div_for_hdmi[402] div = 6
[  372.234512] [hdmitx:] configure venc
[  372.235068] [hdmitx:] config_tv_enc_calc[63] vic = 95
[  372.235850] [hdmitx:] hdmitx_soft_reset[1263]
[  372.236553] [hdmitx:]  config hdmitx IP vic = 95 cd:6 cs: 1
[  372.237381] [hdmitx:] configure hdmitx21
[  372.237983] [hdmitx:] warn: SCDC not present, should not send 1:10
[  372.239957] [hdmitx:] enable phy to dig
[  372.240002] [hdmitx:] hdmitx_set_dispmode[1551] frl_rate 0 htotal 4400 cs 1 cd 6 h_unstable 0
[  372.240080] [hdmitx:] hdmitx_set_drm_pkt: tf=1, cf=1, colormetry=0
[  372.242017] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  372.280701] [hdmitx:] set21_phy_by_mode_s7d[188] rterm = 7
[  372.282067] [hdmitx:] Sink is HDMI device
[  372.282273] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  372.282942] [hdmitx:] set audio
[  372.283384] [hdmitx:] audio_param->chs = 1
[  372.284033] [hdmitx:] aud_src_if = 0
[  372.284646] [hdmitx:] aud_n_para = 5120
[  372.285279] [hdmitx:] audio state: AUDIO_UNMUTE
[  372.285941] [hdmitx:] vinfo: set cur_enc_ppc as 1, vpp color: 0
[  372.287099] DOLBY: vout_notify_callback: VOUT_EVENT_MODE_CHANGE
[  372.287701] vsync_pts_inc 3000 1/30
[  372.288485] [drm] meson_vout_update_mode_name: hdmitx update vout 1 name 2160p30hz.
[  372.302937] [snd-soc]: spdif_a is set to disable
[  372.303016] [snd-soc]: aml_audio_reset, reg 0xa, shift 9, use_vadtop 0
[  372.303296] [snd-soc]: aml_audio_reset, reg 0xa, shift 14, use_vadtop 0
[  372.304286] [snd-soc]: hdmitx src switch to spdif 0
[  372.305018] [snd-soc]: sharebuffer_spdifout_prepare  get_hdmitx_audio_src(rtd->card):0  spdif_id:0
[  372.306279] [hdmitx:] hdmitx_audio_notify_callback[798] audio prepare
[  372.306760] [hdmitx:] hdmitx_set_drm_pkt: tf=16, cf=9, colormetry=0
[  372.307203] [snd-soc]: spdif_a fifo ctrl, frddr:0 type:1, 16 bits, chmask 0x3, swap 0x10
[  372.308130] [hdmitx:] hdmitx_audio_notify_callback[803] type:1 rate:3 size:1 chs:2 i2s_ch_mask:1 aud_src_if:0
[  372.309517] [hdmitx:] aout notify format CT_PCM
[  372.310203] [hdmitx:] set audio
[  372.310741] [hdmitx:] audio_param->chs = 1
[  372.311387] [hdmitx:] aud_src_if = 0
[  372.311975] [hdmitx:] aud_n_para = 5120
[  372.312630] [hdmitx:] audio state: AUDIO_UNMUTE
[  372.313304] [hdmitx:] set audio param
[  372.313985] [snd-soc]: spdif_a is set to enable
[  372.333961] [hdmitx:] avmute_store -1
[  375.716019] [hdmitx:] avmute_store 1
[  375.816322] [hdmitx:] phy_store 0
[  375.973710] [drm] build_hdmitx_attr_str:420,8bit = 3+8
[  375.973940] [drm] [meson_hdmitx_encoder_atomic_disable]
[  375.974617] [drm] am_meson_crtc_atomic_disable-[0]:in
[  375.975553] [hdmitx:] hdmitx_set_drm_pkt: disable drm pkt
[  375.976329] [hdmitx:] TV not support DV, clr dv_vsif
[  375.977015] [hdmitx:] DV H14b VSIF, switching signal to SDR
[  375.977935] [hdmitx:] hdmitx_set_hdr10plus_pkt: null vsif
[  375.978762] [hdmitx:] hdmitx_unregister_vrr ret = 0
[  375.979732] [drm] am_meson_crtc_atomic_enable-[0] in: new[2160p50hz], old[2160p30hz], vmode[4-4], uboot[0]
[  375.980772] [drm] am_meson_crtc_atomic_enable-[0]: enable mode 2160p50hz final vmode 0
[  375.982135] [hdmitx:] set21_s7d_htxpll_clk_out[96] htxpll vco 5940000 div 2
[  375.983232] [hdmitx:] pll_od0 = 1, pll_od2 = 0, pll_od1 = 0
[  375.983667] [hdmitx:] clocks_set_vid_clk_div_for_hdmi[402] div = 6
[  375.984633] [hdmitx:] configure venc
[  375.985155] [hdmitx:] config_tv_enc_calc[63] vic = 96
[  375.985961] [hdmitx:] hdmitx_soft_reset[1263]
[  375.986617] [hdmitx:]  config hdmitx IP vic = 96 cd:4 cs: 3
[  375.987438] [hdmitx:] configure hdmitx21
[  375.988067] [hdmitx:] warn: SCDC not present, should not send 1:10
[  375.990069] [hdmitx:] enable phy to dig
[  375.990121] [hdmitx:] hdmitx_set_dispmode[1551] frl_rate 0 htotal 5280 cs 3 cd 4 h_unstable 0
[  375.990196] [hdmitx:] hdmitx_set_drm_pkt: tf=1, cf=1, colormetry=0
[  375.992133] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  376.028671] [hdmitx:] set21_phy_by_mode_s7d[188] rterm = 7
[  376.030006] [hdmitx:] Sink is HDMI device
[  376.030067] [hdmitx:] clear vsif for non-4k mode.
[  376.030719] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  376.031583] [hdmitx:] set audio
[  376.032044] [hdmitx:] audio_param->chs = 1
[  376.032720] [hdmitx:] aud_src_if = 0
[  376.033282] [hdmitx:] aud_n_para = 5120
[  376.033930] [hdmitx:] audio state: AUDIO_UNMUTE
[  376.034601] [hdmitx:] vinfo: set cur_enc_ppc as 1, vpp color: 0
[  376.035726] DOLBY: vout_notify_callback: VOUT_EVENT_MODE_CHANGE
[  376.036362] vsync_pts_inc 1800 1/50
[  376.036919] [snd-soc]: spdif_a is set to disable
[  376.036996] [snd-soc]: aml_audio_reset, reg 0xa, shift 9, use_vadtop 0
[  376.037200] [drm] meson_vout_update_mode_name: hdmitx update vout 1 name 2160p50hz.
[  376.037885] [snd-soc]: aml_audio_reset, reg 0xa, shift 14, use_vadtop 0
[  376.039978] [snd-soc]: hdmitx src switch to spdif 0
[  376.040725] [snd-soc]: sharebuffer_spdifout_prepare  get_hdmitx_audio_src(rtd->card):0  spdif_id:0
[  376.041966] [hdmitx:] hdmitx_audio_notify_callback[798] audio prepare
[  376.042887] [snd-soc]: spdif_a fifo ctrl, frddr:0 type:1, 16 bits, chmask 0x3, swap 0x10
[  376.042905] [hdmitx:] hdmitx_audio_notify_callback[803] type:1 rate:3 size:1 chs:2 i2s_ch_mask:1 aud_src_if:0
[  376.044261] [hdmitx:] aout notify format CT_PCM
[  376.044984] [hdmitx:] set audio
[  376.045513] [hdmitx:] audio_param->chs = 1
[  376.046152] [hdmitx:] aud_src_if = 0
[  376.046741] [hdmitx:] aud_n_para = 5120
[  376.047398] [hdmitx:] audio state: AUDIO_UNMUTE
[  376.048124] [hdmitx:] set audio param
[  376.048805] [snd-soc]: spdif_a is set to enable
[  376.074955] [hdmitx:] avmute_store -1
[  380.356663] [hdmitx:] avmute_store 1
[  380.456955] [hdmitx:] phy_store 0
[  380.590447] [drm] build_hdmitx_attr_str:422,12bit = 1+12
[  380.590698] [drm] [meson_hdmitx_encoder_atomic_disable]
[  380.591397] [drm] am_meson_crtc_atomic_disable-[0]:in
[  380.592303] [hdmitx:] hdmitx_set_drm_pkt: disable drm pkt
[  380.593052] [hdmitx:] TV not support DV, clr dv_vsif
[  380.593780] [hdmitx:] DV H14b VSIF, switching signal to SDR
[  380.594674] [hdmitx:] hdmitx_set_hdr10plus_pkt: null vsif
[  380.595484] [hdmitx:] hdmitx_unregister_vrr ret = 0
[  380.596118] [drm] am_meson_crtc_atomic_enable-[0] in: new[2160p25hz], old[2160p50hz], vmode[4-4], uboot[0]
[  380.597508] [drm] am_meson_crtc_atomic_enable-[0]: enable mode 2160p25hz final vmode 0
[  380.598906] [hdmitx:] set21_s7d_htxpll_clk_out[96] htxpll vco 5940000 div 2
[  380.599979] [hdmitx:] pll_od0 = 1, pll_od2 = 1, pll_od1 = 2
[  380.600424] [hdmitx:] clocks_set_vid_clk_div_for_hdmi[402] div = 6
[  380.601371] [hdmitx:] configure venc
[  380.601913] [hdmitx:] config_tv_enc_calc[63] vic = 94
[  380.602693] [hdmitx:] hdmitx_soft_reset[1263]
[  380.603377] [hdmitx:]  config hdmitx IP vic = 94 cd:6 cs: 1
[  380.604197] [hdmitx:] configure hdmitx21
[  380.604845] [hdmitx:] warn: SCDC not present, should not send 1:10
[  380.606804] [hdmitx:] enable phy to dig
[  380.606849] [hdmitx:] hdmitx_set_dispmode[1551] frl_rate 0 htotal 5280 cs 1 cd 6 h_unstable 0
[  380.648646] [hdmitx:] set21_phy_by_mode_s7d[188] rterm = 7
[  380.649980] [hdmitx:] Sink is HDMI device
[  380.650121] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  380.650831] [hdmitx:] set audio
[  380.651294] [hdmitx:] audio_param->chs = 1
[  380.651942] [hdmitx:] aud_src_if = 0
[  380.652532] [hdmitx:] aud_n_para = 5120
[  380.653200] [hdmitx:] audio state: AUDIO_UNMUTE
[  380.653852] [hdmitx:] vinfo: set cur_enc_ppc as 1, vpp color: 0
[  380.654952] DOLBY: vout_notify_callback: VOUT_EVENT_MODE_CHANGE
[  380.655610] vsync_pts_inc 3600 1/25
[  380.656360] [drm] meson_vout_update_mode_name: hdmitx update vout 1 name 2160p25hz.
[  380.668879] [snd-soc]: spdif_a is set to disable
[  380.668994] [snd-soc]: aml_audio_reset, reg 0xa, shift 9, use_vadtop 0
[  380.669293] [snd-soc]: aml_audio_reset, reg 0xa, shift 14, use_vadtop 0
[  380.670273] [snd-soc]: hdmitx src switch to spdif 0
[  380.670986] [snd-soc]: sharebuffer_spdifout_prepare  get_hdmitx_audio_src(rtd->card):0  spdif_id:0
[  380.672260] [hdmitx:] hdmitx_audio_notify_callback[798] audio prepare
[  380.673219] [snd-soc]: spdif_a fifo ctrl, frddr:0 type:1, 16 bits, chmask 0x3, swap 0x10
[  380.673234] [hdmitx:] hdmitx_audio_notify_callback[803] type:1 rate:3 size:1 chs:2 i2s_ch_mask:1 aud_src_if:0
[  380.674561] [hdmitx:] aout notify format CT_PCM
[  380.675265] [hdmitx:] set audio
[  380.675802] [hdmitx:] audio_param->chs = 1
[  380.676448] [hdmitx:] aud_src_if = 0
[  380.677049] [hdmitx:] aud_n_para = 5120
[  380.677683] [hdmitx:] audio state: AUDIO_UNMUTE
[  380.678367] [hdmitx:] set audio param
[  380.679049] [snd-soc]: spdif_a is set to enable
[  380.686964] [hdmitx:] hdmitx_set_drm_pkt: tf=16, cf=9, colormetry=0
[  380.715626] [hdmitx:] avmute_store -1
[  384.295261] [hdmitx:] avmute_store 1
[  384.395586] [hdmitx:] phy_store 0
[  384.567212] [drm] [meson_encoder_vrr_change], seamless is 0
[  384.567389] [drm] build_hdmitx_attr_str:422,12bit = 1+12
[  384.568313] [drm] [meson_hdmitx_encoder_atomic_disable]
[  384.569009] [drm] am_meson_crtc_atomic_disable-[0]:in
[  384.569995] [hdmitx:] hdmitx_set_drm_pkt: disable drm pkt
[  384.570686] [hdmitx:] TV not support DV, clr dv_vsif
[  384.571378] [hdmitx:] DV H14b VSIF, switching signal to SDR
[  384.572270] [hdmitx:] hdmitx_set_hdr10plus_pkt: null vsif
[  384.573125] [hdmitx:] hdmitx_unregister_vrr ret = 0
[  384.573718] [drm] am_meson_crtc_atomic_enable-[0] in: new[2160p30hz], old[2160p25hz], vmode[4-4], uboot[0]
[  384.575078] [drm] am_meson_crtc_atomic_enable-[0]: enable mode 2160p30hz final vmode 0
[  384.576465] [hdmitx:] set21_s7d_htxpll_clk_out[96] htxpll vco 5940000 div 2
[  384.577564] [hdmitx:] pll_od0 = 1, pll_od2 = 1, pll_od1 = 2
[  384.578025] [hdmitx:] clocks_set_vid_clk_div_for_hdmi[402] div = 6
[  384.578954] [hdmitx:] configure venc
[  384.579515] [hdmitx:] config_tv_enc_calc[63] vic = 95
[  384.580294] [hdmitx:] hdmitx_soft_reset[1263]
[  384.581021] [hdmitx:]  config hdmitx IP vic = 95 cd:6 cs: 1
[  384.581800] [hdmitx:] configure hdmitx21
[  384.582429] [hdmitx:] warn: SCDC not present, should not send 1:10
[  384.584448] [hdmitx:] enable phy to dig
[  384.584502] [hdmitx:] hdmitx_set_dispmode[1551] frl_rate 0 htotal 4400 cs 1 cd 6 h_unstable 0
[  384.584572] [hdmitx:] hdmitx_set_drm_pkt: tf=1, cf=1, colormetry=0
[  384.586513] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  384.624658] [hdmitx:] set21_phy_by_mode_s7d[188] rterm = 7
[  384.626001] [hdmitx:] Sink is HDMI device
[  384.626200] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  384.626887] [hdmitx:] set audio
[  384.627314] [hdmitx:] audio_param->chs = 1
[  384.627962] [hdmitx:] aud_src_if = 0
[  384.628552] [hdmitx:] aud_n_para = 5120
[  384.629246] [hdmitx:] audio state: AUDIO_UNMUTE
[  384.629875] [hdmitx:] vinfo: set cur_enc_ppc as 1, vpp color: 0
[  384.631051] DOLBY: vout_notify_callback: VOUT_EVENT_MODE_CHANGE
[  384.631631] vsync_pts_inc 3000 1/30
[  384.632442] [drm] meson_vout_update_mode_name: hdmitx update vout 1 name 2160p30hz.
[  384.651265] [hdmitx:] hdmitx_set_drm_pkt: tf=16, cf=9, colormetry=0
[  384.658121] [snd-soc]: spdif_a is set to disable
[  384.658187] [snd-soc]: aml_audio_reset, reg 0xa, shift 9, use_vadtop 0
[  384.658463] [snd-soc]: aml_audio_reset, reg 0xa, shift 14, use_vadtop 0
[  384.659449] [snd-soc]: hdmitx src switch to spdif 0
[  384.660170] [snd-soc]: sharebuffer_spdifout_prepare  get_hdmitx_audio_src(rtd->card):0  spdif_id:0
[  384.661473] [hdmitx:] hdmitx_audio_notify_callback[798] audio prepare
[  384.662369] [snd-soc]: spdif_a fifo ctrl, frddr:0 type:1, 16 bits, chmask 0x3, swap 0x10
[  384.662378] [hdmitx:] hdmitx_audio_notify_callback[803] type:1 rate:3 size:1 chs:2 i2s_ch_mask:1 aud_src_if:0
[  384.663744] [hdmitx:] aout notify format CT_PCM
[  384.664448] [hdmitx:] set audio
[  384.664998] [hdmitx:] audio_param->chs = 1
[  384.665632] [hdmitx:] aud_src_if = 0
[  384.666220] [hdmitx:] aud_n_para = 5120
[  384.666856] [hdmitx:] audio state: AUDIO_UNMUTE
[  384.667550] [hdmitx:] set audio param
[  384.668227] [snd-soc]: spdif_a is set to enable
[  384.675934] [hdmitx:] avmute_store -1
[  386.024638] [aml_send_sync_trace 4388] sync token[36944]
[  386.024662] >>> aml_send_msg()
[  386.025688] ipc_sdio_host_msgack_handler 000000007f97c8b3
[  386.026118] [aml_msgackind 2039] msg ack hostid=0xffffff804626a300
[  386.027026] [cmd_mgr_llind         329] cmd tkn[43]  flags:0008  result: -4  cmd: 105-MM_SYNC_TRACE            - reqcfm(   0-none)
[  386.028656] [cmd_complete           65] cmd tkn[43]  flags:0000  result: -4  cmd: 105-MM_SYNC_TRACE            - reqcfm(   0-none)
[  394.267273] [SP FRAME RX] arp req,vif_idx:0 sender:[f8:8c:21:8f:40:25 192.168.0.1]receiver:[00:00:00:00:00:00 192.168.0.108]
[  394.268260] [SP FRAME TX] arp rsp,vif_idx:0 sender:[c0:e3:50:49:af:ae 192.168.0.108]receiver:[f8:8c:21:8f:40:25 192.168.0.1]
[  394.867970] type=1400 audit(1753189712.087:1216): avc:  denied  { read } for  comm="adbd" path="socket:[34862]" dev="sockfs" ino=34862 scontext=u:r:su:s0 tcontext=u:r:su:s0 tclass=tcp_socket permissive=1
[  394.870035] type=1400 audit(1753189712.087:1217): avc:  denied  { write } for  comm="adbd" path="socket:[34862]" dev="sockfs" ino=34862 scontext=u:r:su:s0 tcontext=u:r:su:s0 tclass=tcp_socket permissive=1
[  401.888611] type=1400 audit(1753189719.107:1218): avc:  denied  { search } for  comm="sh" name="0" dev="tmpfs" ino=13 scontext=u:r:su:s0 tcontext=u:object_r:mnt_user_file:s0 tclass=dir permissive=1
[  401.890703] type=1400 audit(1753189719.107:1219): avc:  denied  { read } for  comm="sh" name="primary" dev="tmpfs" ino=42 scontext=u:r:su:s0 tcontext=u:object_r:mnt_user_file:s0 tclass=lnk_file permissive=1
[  401.892879] type=1400 audit(1753189719.111:1220): avc:  denied  { search } for  comm="sh" name="/" dev="fuse" ino=131 scontext=u:r:su:s0 tcontext=u:object_r:fuse:s0 tclass=dir permissive=1
[  422.488179] type=1400 audit(1753189739.707:1221): avc:  denied  { getattr } for  comm="sh" path="/system/bin/toybox" dev="dm-8" ino=27555588 scontext=u:r:su:s0 tcontext=u:object_r:toolbox_exec:s0 tclass=file permissive=1
[  422.490361] type=1400 audit(1753189739.707:1222): avc:  denied  { execute } for  comm="sh" name="toybox" dev="dm-8" ino=27555588 scontext=u:r:su:s0 tcontext=u:object_r:toolbox_exec:s0 tclass=file permissive=1
[  422.493036] type=1400 audit(1753189739.711:1223): avc:  denied  { read open } for  comm="sh" path="/system/bin/toybox" dev="dm-8" ino=27555588 scontext=u:r:su:s0 tcontext=u:object_r:toolbox_exec:s0 tclass=file permissive=1
[  422.495294] type=1400 audit(1753189739.711:1224): avc:  denied  { execute_no_trans } for  comm="sh" path="/system/bin/toybox" dev="dm-8" ino=27555588 scontext=u:r:su:s0 tcontext=u:object_r:toolbox_exec:s0 tclass=file permissive=1
[  422.497970] type=1400 audit(1753189739.711:1225): avc:  denied  { map } for  comm="ls" path="/system/bin/toybox" dev="dm-8" ino=27555588 scontext=u:r:su:s0 tcontext=u:object_r:toolbox_exec:s0 tclass=file permissive=1
[  422.511487] type=1400 audit(1753189739.731:1226): avc:  denied  { read } for  comm="ls" name="0" dev="fuse" ino=1408 scontext=u:r:su:s0 tcontext=u:object_r:fuse:s0 tclass=dir permissive=1
[  422.513317] type=1400 audit(1753189739.731:1227): avc:  denied  { open } for  comm="ls" path="/storage/emulated/0" dev="fuse" ino=1408 scontext=u:r:su:s0 tcontext=u:object_r:fuse:s0 tclass=dir permissive=1
[  422.513554] audit: audit_lost=288 audit_rate_limit=5 audit_backlog_limit=64
[  422.516635] audit: rate limit exceeded
[  426.576619] type=1400 audit(1753189743.795:1229): avc:  denied  { write } for  comm="rm" name="1.log" dev="fuse" ino=5184 scontext=u:r:su:s0 tcontext=u:object_r:fuse:s0 tclass=file permissive=1
[  426.578445] type=1400 audit(1753189743.795:1230): avc:  denied  { write } for  comm="rm" name="0" dev="fuse" ino=1408 scontext=u:r:su:s0 tcontext=u:object_r:fuse:s0 tclass=dir permissive=1
[  426.580544] type=1400 audit(1753189743.795:1231): avc:  denied  { remove_name } for  comm="rm" name="1.log" dev="fuse" ino=5184 scontext=u:r:su:s0 tcontext=u:object_r:fuse:s0 tclass=dir permissive=1
[  429.804674] [SP FRAME TX] arp req,vif_idx:0 sender:[c0:e3:50:49:af:ae 192.168.0.108]receiver:[00:00:00:00:00:00 192.168.0.1]
[  429.807186] [SP FRAME RX] arp rsp,vif_idx:0 sender:[f8:8c:21:8f:40:25 192.168.0.1]receiver:[c0:e3:50:49:af:ae 192.168.0.108]
[  437.477356] type=1400 audit(1753189754.699:1233): avc:  denied  { execute } for  comm="sh" name="logcat" dev="dm-8" ino=27552265 scontext=u:r:su:s0 tcontext=u:object_r:logcat_exec:s0 tclass=file permissive=1
[  437.479867] type=1400 audit(1753189754.699:1234): avc:  denied  { open } for  comm="sh" path="/system/bin/logcat" dev="dm-8" ino=27552265 scontext=u:r:su:s0 tcontext=u:object_r:logcat_exec:s0 tclass=file permissive=1
[  437.482033] type=1400 audit(1753189754.699:1235): avc:  denied  { execute_no_trans } for  comm="sh" path="/system/bin/logcat" dev="dm-8" ino=27552265 scontext=u:r:su:s0 tcontext=u:object_r:logcat_exec:s0 tclass=file permissive=1
[  437.484944] type=1400 audit(1753189754.699:1236): avc:  denied  { map } for  comm="logcat" path="/system/bin/logcat" dev="dm-8" ino=27552265 scontext=u:r:su:s0 tcontext=u:object_r:logcat_exec:s0 tclass=file permissive=1
[  437.496466] type=1400 audit(1753189754.715:1237): avc:  denied  { connectto } for  comm="logcat" path="/dev/socket/logd" scontext=u:r:su:s0 tcontext=u:r:logd:s0 tclass=unix_stream_socket permissive=1
[  437.500824] audit: audit_lost=289 audit_rate_limit=5 audit_backlog_limit=64
[  437.501163] audit: rate limit exceeded
[  437.501450] type=1400 audit(1753189754.723:1238): avc:  denied  { add_name } for  comm="sh" name="1.log" scontext=u:r:su:s0 tcontext=u:object_r:fuse:s0 tclass=dir permissive=1
[  437.522332] logd: logdr: UID=0 GID=0 PID=4405 b tail=0 logMask=99 pid=0 start=0ns deadline=0ns
[  440.459994] [hdmitx:] avmute_store 1
[  440.560325] [hdmitx:] phy_store 0
[  440.718287] [drm] [meson_encoder_vrr_change], seamless is 0
[  440.718463] [drm] build_hdmitx_attr_str:422,12bit = 1+12
[  440.719350] [drm] [meson_hdmitx_encoder_atomic_disable]
[  440.720051] [drm] am_meson_crtc_atomic_disable-[0]:in
[  440.720960] [hdmitx:] hdmitx_set_drm_pkt: disable drm pkt
[  440.721737] [hdmitx:] TV not support DV, clr dv_vsif
[  440.722437] [hdmitx:] DV H14b VSIF, switching signal to SDR
[  440.723318] [hdmitx:] hdmitx_set_hdr10plus_pkt: null vsif
[  440.724133] [hdmitx:] hdmitx_unregister_vrr ret = 0
[  440.724818] [drm] am_meson_crtc_atomic_enable-[0] in: new[2160p25hz], old[2160p30hz], vmode[4-4], uboot[0]
[  440.726167] [drm] am_meson_crtc_atomic_enable-[0]: enable mode 2160p25hz final vmode 0
[  440.727564] [hdmitx:] set21_s7d_htxpll_clk_out[96] htxpll vco 5940000 div 2
[  440.728871] [hdmitx:] pll_od0 = 1, pll_od2 = 1, pll_od1 = 2
[  440.729101] [hdmitx:] clocks_set_vid_clk_div_for_hdmi[402] div = 6
[  440.730034] [hdmitx:] configure venc
[  440.730591] [hdmitx:] config_tv_enc_calc[63] vic = 94
[  440.731373] [hdmitx:] hdmitx_soft_reset[1263]
[  440.732137] [hdmitx:]  config hdmitx IP vic = 94 cd:6 cs: 1
[  440.732911] [hdmitx:] configure hdmitx21
[  440.733509] [hdmitx:] warn: SCDC not present, should not send 1:10
[  440.735492] [hdmitx:] enable phy to dig
[  440.735534] [hdmitx:] hdmitx_set_dispmode[1551] frl_rate 0 htotal 5280 cs 1 cd 6 h_unstable 0
[  440.735629] [hdmitx:] hdmitx_set_drm_pkt: tf=1, cf=1, colormetry=0
[  440.737548] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  440.772639] [hdmitx:] set21_phy_by_mode_s7d[188] rterm = 7
[  440.773998] [hdmitx:] Sink is HDMI device
[  440.774203] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  440.774871] [hdmitx:] set audio
[  440.775314] [hdmitx:] audio_param->chs = 1
[  440.775963] [hdmitx:] aud_src_if = 0
[  440.776552] [hdmitx:] aud_n_para = 5120
[  440.777238] [hdmitx:] audio state: AUDIO_UNMUTE
[  440.777872] [hdmitx:] vinfo: set cur_enc_ppc as 1, vpp color: 0
[  440.779019] DOLBY: vout_notify_callback: VOUT_EVENT_MODE_CHANGE
[  440.779630] vsync_pts_inc 3600 1/25
[  440.780402] [drm] meson_vout_update_mode_name: hdmitx update vout 1 name 2160p25hz.
[  440.808452] [snd-soc]: spdif_a is set to disable
[  440.808517] [snd-soc]: aml_audio_reset, reg 0xa, shift 9, use_vadtop 0
[  440.808819] [snd-soc]: aml_audio_reset, reg 0xa, shift 14, use_vadtop 0
[  440.809779] [snd-soc]: hdmitx src switch to spdif 0
[  440.810499] [snd-soc]: sharebuffer_spdifout_prepare  get_hdmitx_audio_src(rtd->card):0  spdif_id:0
[  440.811771] [hdmitx:] hdmitx_audio_notify_callback[798] audio prepare
[  440.812712] [snd-soc]: spdif_a fifo ctrl, frddr:0 type:1, 16 bits, chmask 0x3, swap 0x10
[  440.812722] [hdmitx:] hdmitx_audio_notify_callback[803] type:1 rate:3 size:1 chs:2 i2s_ch_mask:1 aud_src_if:0
[  440.814076] [hdmitx:] aout notify format CT_PCM
[  440.814780] [hdmitx:] set audio
[  440.815316] [hdmitx:] audio_param->chs = 1
[  440.815619] [hdmitx:] hdmitx_set_drm_pkt: tf=16, cf=9, colormetry=0
[  440.815961] [hdmitx:] aud_src_if = 0
[  440.817471] [hdmitx:] aud_n_para = 5120
[  440.818107] [hdmitx:] audio state: AUDIO_UNMUTE
[  440.818790] [hdmitx:] set audio param
[  440.819480] [snd-soc]: spdif_a is set to enable
[  440.840739] [hdmitx:] avmute_store -1
[  444.947361] [hdmitx:] avmute_store 1
[  445.047639] [hdmitx:] phy_store 0
[  445.215914] [drm] [meson_encoder_vrr_change], seamless is 0
[  445.216091] [drm] build_hdmitx_attr_str:422,12bit = 1+12
[  445.217290] [drm] [meson_hdmitx_encoder_atomic_disable]
[  445.217695] [drm] am_meson_crtc_atomic_disable-[0]:in
[  445.218572] [hdmitx:] hdmitx_set_drm_pkt: disable drm pkt
[  445.219363] [hdmitx:] TV not support DV, clr dv_vsif
[  445.220065] [hdmitx:] DV H14b VSIF, switching signal to SDR
[  445.220971] [hdmitx:] hdmitx_set_hdr10plus_pkt: null vsif
[  445.221764] [hdmitx:] hdmitx_unregister_vrr ret = 0
[  445.222420] [drm] am_meson_crtc_atomic_enable-[0] in: new[2160p30hz], old[2160p25hz], vmode[4-4], uboot[0]
[  445.223801] [drm] am_meson_crtc_atomic_enable-[0]: enable mode 2160p30hz final vmode 0
[  445.225222] [hdmitx:] set21_s7d_htxpll_clk_out[96] htxpll vco 5940000 div 2
[  445.226255] [hdmitx:] pll_od0 = 1, pll_od2 = 1, pll_od1 = 2
[  445.226728] [hdmitx:] clocks_set_vid_clk_div_for_hdmi[402] div = 6
[  445.227658] [hdmitx:] configure venc
[  445.228402] [hdmitx:] config_tv_enc_calc[63] vic = 95
[  445.229051] [hdmitx:] hdmitx_soft_reset[1263]
[  445.229708] [hdmitx:]  config hdmitx IP vic = 95 cd:6 cs: 1
[  445.230503] [hdmitx:] configure hdmitx21
[  445.231133] [hdmitx:] warn: SCDC not present, should not send 1:10
[  445.233157] [hdmitx:] enable phy to dig
[  445.233303] [hdmitx:] hdmitx_set_drm_pkt: tf=1, cf=1, colormetry=0
[  445.234174] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  445.235706] [hdmitx:] hdmitx_set_dispmode[1551] frl_rate 0 htotal 4400 cs 1 cd 6 h_unstable 0
[  445.276653] [hdmitx:] set21_phy_by_mode_s7d[188] rterm = 7
[  445.277967] [hdmitx:] Sink is HDMI device
[  445.278087] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  445.278793] [hdmitx:] set audio
[  445.279275] [hdmitx:] audio_param->chs = 1
[  445.279924] [hdmitx:] aud_src_if = 0
[  445.280512] [hdmitx:] aud_n_para = 5120
[  445.281166] [hdmitx:] audio state: AUDIO_UNMUTE
[  445.281834] [hdmitx:] vinfo: set cur_enc_ppc as 1, vpp color: 0
[  445.282920] DOLBY: vout_notify_callback: VOUT_EVENT_MODE_CHANGE
[  445.283593] vsync_pts_inc 3000 1/30
[  445.284325] [drm] meson_vout_update_mode_name: hdmitx update vout 1 name 2160p30hz.
[  445.299989] [hdmitx:] hdmitx_set_drm_pkt: tf=16, cf=9, colormetry=0
[  445.312447] [snd-soc]: spdif_a is set to disable
[  445.312542] [snd-soc]: aml_audio_reset, reg 0xa, shift 9, use_vadtop 0
[  445.312854] [snd-soc]: aml_audio_reset, reg 0xa, shift 14, use_vadtop 0
[  445.313832] [snd-soc]: hdmitx src switch to spdif 0
[  445.314531] [snd-soc]: sharebuffer_spdifout_prepare  get_hdmitx_audio_src(rtd->card):0  spdif_id:0
[  445.315806] [hdmitx:] hdmitx_audio_notify_callback[798] audio prepare
[  445.316795] [snd-soc]: spdif_a fifo ctrl, frddr:0 type:1, 16 bits, chmask 0x3, swap 0x10
[  445.316811] [hdmitx:] hdmitx_audio_notify_callback[803] type:1 rate:3 size:1 chs:2 i2s_ch_mask:1 aud_src_if:0
[  445.318105] [hdmitx:] aout notify format CT_PCM
[  445.318808] [hdmitx:] set audio
[  445.319346] [hdmitx:] audio_param->chs = 1
[  445.319991] [hdmitx:] aud_src_if = 0
[  445.320595] [hdmitx:] aud_n_para = 5120
[  445.321220] [hdmitx:] audio state: AUDIO_UNMUTE
[  445.321901] [hdmitx:] set audio param
[  445.322586] [snd-soc]: spdif_a is set to enable
[  445.327588] [hdmitx:] avmute_store -1
[  447.464627] [aml_send_sync_trace 4388] sync token[36945]
[  447.464653] >>> aml_send_msg()
[  447.465572] ipc_sdio_host_msgack_handler 0000000098820be5
[  447.466109] [aml_msgackind 2039] msg ack hostid=0xffffff8081c45f80
[  447.467017] [cmd_mgr_llind         329] cmd tkn[44]  flags:0008  result: -4  cmd: 105-MM_SYNC_TRACE            - reqcfm(   0-none)
[  447.468636] [cmd_complete           65] cmd tkn[44]  flags:0000  result: -4  cmd: 105-MM_SYNC_TRACE            - reqcfm(   0-none)
[  449.610094] [hdmitx:] avmute_store 1
[  449.710389] [hdmitx:] phy_store 0
[  449.866884] [drm] [meson_encoder_vrr_change], seamless is 0
[  449.867056] [drm] build_hdmitx_attr_str:422,12bit = 1+12
[  449.867965] [drm] [meson_hdmitx_encoder_atomic_disable]
[  449.868668] [drm] am_meson_crtc_atomic_disable-[0]:in
[  449.869544] [hdmitx:] hdmitx_set_drm_pkt: disable drm pkt
[  449.870325] [hdmitx:] TV not support DV, clr dv_vsif
[  449.871031] [hdmitx:] DV H14b VSIF, switching signal to SDR
[  449.871939] [hdmitx:] hdmitx_set_hdr10plus_pkt: null vsif
[  449.872781] [hdmitx:] hdmitx_unregister_vrr ret = 0
[  449.873388] [drm] am_meson_crtc_atomic_enable-[0] in: new[2160p25hz], old[2160p30hz], vmode[4-4], uboot[0]
[  449.874751] [drm] am_meson_crtc_atomic_enable-[0]: enable mode 2160p25hz final vmode 0
[  449.876174] [hdmitx:] set21_s7d_htxpll_clk_out[96] htxpll vco 5940000 div 2
[  449.877256] [hdmitx:] pll_od0 = 1, pll_od2 = 1, pll_od1 = 2
[  449.877693] [hdmitx:] clocks_set_vid_clk_div_for_hdmi[402] div = 6
[  449.878629] [hdmitx:] configure venc
[  449.879185] [hdmitx:] config_tv_enc_calc[63] vic = 94
[  449.879967] [hdmitx:] hdmitx_soft_reset[1263]
[  449.880673] [hdmitx:]  config hdmitx IP vic = 94 cd:6 cs: 1
[  449.881470] [hdmitx:] configure hdmitx21
[  449.882100] [hdmitx:] warn: SCDC not present, should not send 1:10
[  449.884090] [hdmitx:] enable phy to dig
[  449.884144] [hdmitx:] hdmitx_set_dispmode[1551] frl_rate 0 htotal 5280 cs 1 cd 6 h_unstable 0
[  449.884218] [hdmitx:] hdmitx_set_drm_pkt: tf=1, cf=1, colormetry=0
[  449.886156] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  449.924660] [hdmitx:] set21_phy_by_mode_s7d[188] rterm = 7
[  449.926134] [hdmitx:] Sink is HDMI device
[  449.926308] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  449.927091] [hdmitx:] set audio
[  449.927521] [hdmitx:] audio_param->chs = 1
[  449.928179] [hdmitx:] aud_src_if = 0
[  449.928941] [hdmitx:] aud_n_para = 5120
[  449.929340] [hdmitx:] audio state: AUDIO_UNMUTE
[  449.930022] [hdmitx:] vinfo: set cur_enc_ppc as 1, vpp color: 0
[  449.931182] DOLBY: vout_notify_callback: VOUT_EVENT_MODE_CHANGE
[  449.931777] vsync_pts_inc 3600 1/25
[  449.932510] [drm] meson_vout_update_mode_name: hdmitx update vout 1 name 2160p25hz.
[  449.943482] [snd-soc]: spdif_a is set to disable
[  449.943545] [snd-soc]: aml_audio_reset, reg 0xa, shift 9, use_vadtop 0
[  449.943820] [snd-soc]: aml_audio_reset, reg 0xa, shift 14, use_vadtop 0
[  449.944834] [snd-soc]: hdmitx src switch to spdif 0
[  449.945528] [snd-soc]: sharebuffer_spdifout_prepare  get_hdmitx_audio_src(rtd->card):0  spdif_id:0
[  449.946800] [hdmitx:] hdmitx_audio_notify_callback[798] audio prepare
[  449.947727] [snd-soc]: spdif_a fifo ctrl, frddr:0 type:1, 16 bits, chmask 0x3, swap 0x10
[  449.947737] [hdmitx:] hdmitx_audio_notify_callback[803] type:1 rate:3 size:1 chs:2 i2s_ch_mask:1 aud_src_if:0
[  449.949130] [hdmitx:] aout notify format CT_PCM
[  449.949808] [hdmitx:] set audio
[  449.950347] [hdmitx:] audio_param->chs = 1
[  449.950991] [hdmitx:] aud_src_if = 0
[  449.951580] [hdmitx:] aud_n_para = 5120
[  449.952227] [hdmitx:] audio state: AUDIO_UNMUTE
[  449.952936] [hdmitx:] set audio param
[  449.953600] [snd-soc]: spdif_a is set to enable
[  449.964237] [hdmitx:] hdmitx_set_drm_pkt: tf=16, cf=9, colormetry=0
[  449.989619] [hdmitx:] avmute_store -1
[  453.851848] [hdmitx:] avmute_store 1
[  453.952145] [hdmitx:] phy_store 0
[  454.124651] [drm] [meson_encoder_vrr_change], seamless is 0
[  454.124827] [drm] build_hdmitx_attr_str:422,12bit = 1+12
[  454.125732] [drm] [meson_hdmitx_encoder_atomic_disable]
[  454.126418] [drm] am_meson_crtc_atomic_disable-[0]:in
[  454.127329] [hdmitx:] hdmitx_set_drm_pkt: disable drm pkt
[  454.128129] [hdmitx:] TV not support DV, clr dv_vsif
[  454.128817] [hdmitx:] DV H14b VSIF, switching signal to SDR
[  454.129781] [hdmitx:] hdmitx_set_hdr10plus_pkt: null vsif
[  454.130582] [hdmitx:] hdmitx_unregister_vrr ret = 0
[  454.131173] [drm] am_meson_crtc_atomic_enable-[0] in: new[2160p30hz], old[2160p25hz], vmode[4-4], uboot[0]
[  454.132543] [drm] am_meson_crtc_atomic_enable-[0]: enable mode 2160p30hz final vmode 0
[  454.134078] [hdmitx:] set21_s7d_htxpll_clk_out[96] htxpll vco 5940000 div 2
[  454.135292] [hdmitx:] pll_od0 = 1, pll_od2 = 1, pll_od1 = 2
[  454.135466] [hdmitx:] clocks_set_vid_clk_div_for_hdmi[402] div = 6
[  454.136396] [hdmitx:] configure venc
[  454.136992] [hdmitx:] config_tv_enc_calc[63] vic = 95
[  454.137737] [hdmitx:] hdmitx_soft_reset[1263]
[  454.138419] [hdmitx:]  config hdmitx IP vic = 95 cd:6 cs: 1
[  454.139238] [hdmitx:] configure hdmitx21
[  454.139868] [hdmitx:] warn: SCDC not present, should not send 1:10
[  454.141847] [hdmitx:] enable phy to dig
[  454.141886] [hdmitx:] hdmitx_set_dispmode[1551] frl_rate 0 htotal 4400 cs 1 cd 6 h_unstable 0
[  454.141969] [hdmitx:] hdmitx_set_drm_pkt: tf=1, cf=1, colormetry=0
[  454.143902] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  454.184634] [hdmitx:] set21_phy_by_mode_s7d[188] rterm = 7
[  454.185967] [hdmitx:] Sink is HDMI device
[  454.186126] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  454.186813] [hdmitx:] set audio
[  454.187276] [hdmitx:] audio_param->chs = 1
[  454.187923] [hdmitx:] aud_src_if = 0
[  454.188512] [hdmitx:] aud_n_para = 5120
[  454.189189] [hdmitx:] audio state: AUDIO_UNMUTE
[  454.189838] [hdmitx:] vinfo: set cur_enc_ppc as 1, vpp color: 0
[  454.190947] DOLBY: vout_notify_callback: VOUT_EVENT_MODE_CHANGE
[  454.191591] vsync_pts_inc 3000 1/30
[  454.192320] [drm] meson_vout_update_mode_name: hdmitx update vout 1 name 2160p30hz.
[  454.208656] [hdmitx:] hdmitx_set_drm_pkt: tf=16, cf=9, colormetry=0
[  454.220924] [snd-soc]: spdif_a is set to disable
[  454.220992] [snd-soc]: aml_audio_reset, reg 0xa, shift 9, use_vadtop 0
[  454.221267] [snd-soc]: aml_audio_reset, reg 0xa, shift 14, use_vadtop 0
[  454.222251] [snd-soc]: hdmitx src switch to spdif 0
[  454.222973] [snd-soc]: sharebuffer_spdifout_prepare  get_hdmitx_audio_src(rtd->card):0  spdif_id:0
[  454.224245] [hdmitx:] hdmitx_audio_notify_callback[798] audio prepare
[  454.225195] [snd-soc]: spdif_a fifo ctrl, frddr:0 type:1, 16 bits, chmask 0x3, swap 0x10
[  454.225205] [hdmitx:] hdmitx_audio_notify_callback[803] type:1 rate:3 size:1 chs:2 i2s_ch_mask:1 aud_src_if:0
[  454.226548] [hdmitx:] aout notify format CT_PCM
[  454.227252] [hdmitx:] set audio
[  454.227788] [hdmitx:] audio_param->chs = 1
[  454.228435] [hdmitx:] aud_src_if = 0
[  454.229036] [hdmitx:] aud_n_para = 5120
[  454.229660] [hdmitx:] audio state: AUDIO_UNMUTE
[  454.230355] [hdmitx:] set audio param
[  454.231044] [snd-soc]: spdif_a is set to enable
[  454.235025] [hdmitx:] avmute_store -1
[  458.115687] [hdmitx:] avmute_store 1
[  458.216001] [hdmitx:] phy_store 0
[  458.375550] [drm] [meson_encoder_vrr_change], seamless is 0
[  458.375722] [drm] build_hdmitx_attr_str:422,12bit = 1+12
[  458.376642] [drm] [meson_hdmitx_encoder_atomic_disable]
[  458.377313] [drm] am_meson_crtc_atomic_disable-[0]:in
[  458.378198] [hdmitx:] hdmitx_set_drm_pkt: disable drm pkt
[  458.378994] [hdmitx:] TV not support DV, clr dv_vsif
[  458.379697] [hdmitx:] DV H14b VSIF, switching signal to SDR
[  458.380636] [hdmitx:] hdmitx_set_hdr10plus_pkt: null vsif
[  458.381424] [hdmitx:] hdmitx_unregister_vrr ret = 0
[  458.382055] [drm] am_meson_crtc_atomic_enable-[0] in: new[2160p25hz], old[2160p30hz], vmode[4-4], uboot[0]
[  458.383419] [drm] am_meson_crtc_atomic_enable-[0]: enable mode 2160p25hz final vmode 0
[  458.384892] [hdmitx:] set21_s7d_htxpll_clk_out[96] htxpll vco 5940000 div 2
[  458.385903] [hdmitx:] pll_od0 = 1, pll_od2 = 1, pll_od1 = 2
[  458.386361] [hdmitx:] clocks_set_vid_clk_div_for_hdmi[402] div = 6
[  458.387295] [hdmitx:] configure venc
[  458.387851] [hdmitx:] config_tv_enc_calc[63] vic = 94
[  458.388711] [hdmitx:] hdmitx_soft_reset[1263]
[  458.389322] [hdmitx:]  config hdmitx IP vic = 94 cd:6 cs: 1
[  458.390135] [hdmitx:] configure hdmitx21
[  458.390765] [hdmitx:] warn: SCDC not present, should not send 1:10
[  458.392739] [hdmitx:] enable phy to dig
[  458.392790] [hdmitx:] hdmitx_set_dispmode[1551] frl_rate 0 htotal 5280 cs 1 cd 6 h_unstable 0
[  458.392865] [hdmitx:] hdmitx_set_drm_pkt: tf=1, cf=1, colormetry=0
[  458.394802] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  458.432659] [hdmitx:] set21_phy_by_mode_s7d[188] rterm = 7
[  458.434053] [hdmitx:] Sink is HDMI device
[  458.434272] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  458.434939] [hdmitx:] set audio
[  458.435380] [hdmitx:] audio_param->chs = 1
[  458.436026] [hdmitx:] aud_src_if = 0
[  458.436640] [hdmitx:] aud_n_para = 5120
[  458.437255] [hdmitx:] audio state: AUDIO_UNMUTE
[  458.437938] [hdmitx:] vinfo: set cur_enc_ppc as 1, vpp color: 0
[  458.439022] DOLBY: vout_notify_callback: VOUT_EVENT_MODE_CHANGE
[  458.439694] vsync_pts_inc 3600 1/25
[  458.440422] [drm] meson_vout_update_mode_name: hdmitx update vout 1 name 2160p25hz.
[  458.465862] [snd-soc]: spdif_a is set to disable
[  458.465923] [snd-soc]: aml_audio_reset, reg 0xa, shift 9, use_vadtop 0
[  458.466198] [snd-soc]: aml_audio_reset, reg 0xa, shift 14, use_vadtop 0
[  458.467192] [snd-soc]: hdmitx src switch to spdif 0
[  458.467905] [snd-soc]: sharebuffer_spdifout_prepare  get_hdmitx_audio_src(rtd->card):0  spdif_id:0
[  458.469264] [hdmitx:] hdmitx_audio_notify_callback[798] audio prepare
[  458.470110] [snd-soc]: spdif_a fifo ctrl, frddr:0 type:1, 16 bits, chmask 0x3, swap 0x10
[  458.470123] [hdmitx:] hdmitx_audio_notify_callback[803] type:1 rate:3 size:1 chs:2 i2s_ch_mask:1 aud_src_if:0
[  458.471482] [hdmitx:] aout notify format CT_PCM
[  458.472184] [hdmitx:] set audio
[  458.472740] [hdmitx:] audio_param->chs = 1
[  458.472877] [hdmitx:] hdmitx_set_drm_pkt: tf=16, cf=9, colormetry=0
[  458.473368] [hdmitx:] aud_src_if = 0
[  458.474880] [hdmitx:] aud_n_para = 5120
[  458.475515] [hdmitx:] audio state: AUDIO_UNMUTE
[  458.476197] [hdmitx:] set audio param
[  458.476914] [snd-soc]: spdif_a is set to enable
[  458.500439] [hdmitx:] avmute_store -1
[  462.802849] [hdmitx:] avmute_store 1
[  462.828661] [SP FRAME TX] arp req,vif_idx:0 sender:[c0:e3:50:49:af:ae 192.168.0.108]receiver:[00:00:00:00:00:00 192.168.0.1]
[  462.832018] [SP FRAME RX] arp rsp,vif_idx:0 sender:[f8:8c:21:8f:40:25 192.168.0.1]receiver:[c0:e3:50:49:af:ae 192.168.0.108]
[  462.903174] [hdmitx:] phy_store 0
[  463.073207] [drm] [meson_encoder_vrr_change], seamless is 0
[  463.073386] [drm] build_hdmitx_attr_str:422,12bit = 1+12
[  463.074291] [drm] [meson_hdmitx_encoder_atomic_disable]
[  463.074975] [drm] am_meson_crtc_atomic_disable-[0]:in
[  463.075920] [hdmitx:] hdmitx_set_drm_pkt: disable drm pkt
[  463.076682] [hdmitx:] TV not support DV, clr dv_vsif
[  463.077363] [hdmitx:] DV H14b VSIF, switching signal to SDR
[  463.078241] [hdmitx:] hdmitx_set_hdr10plus_pkt: null vsif
[  463.079068] [hdmitx:] hdmitx_unregister_vrr ret = 0
[  463.079718] [drm] am_meson_crtc_atomic_enable-[0] in: new[2160p30hz], old[2160p25hz], vmode[4-4], uboot[0]
[  463.081091] [drm] am_meson_crtc_atomic_enable-[0]: enable mode 2160p30hz final vmode 0
[  463.082457] [hdmitx:] set21_s7d_htxpll_clk_out[96] htxpll vco 5940000 div 2
[  463.083531] [hdmitx:] pll_od0 = 1, pll_od2 = 1, pll_od1 = 2
[  463.084022] [hdmitx:] clocks_set_vid_clk_div_for_hdmi[402] div = 6
[  463.084970] [hdmitx:] configure venc
[  463.085513] [hdmitx:] config_tv_enc_calc[63] vic = 95
[  463.086295] [hdmitx:] hdmitx_soft_reset[1263]
[  463.086982] [hdmitx:]  config hdmitx IP vic = 95 cd:6 cs: 1
[  463.087797] [hdmitx:] configure hdmitx21
[  463.088427] [hdmitx:] warn: SCDC not present, should not send 1:10
[  463.090445] [hdmitx:] enable phy to dig
[  463.090504] [hdmitx:] hdmitx_set_dispmode[1551] frl_rate 0 htotal 4400 cs 1 cd 6 h_unstable 0
[  463.090579] [hdmitx:] hdmitx_set_drm_pkt: tf=1, cf=1, colormetry=0
[  463.092515] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  463.132653] [hdmitx:] set21_phy_by_mode_s7d[188] rterm = 7
[  463.133975] [hdmitx:] Sink is HDMI device
[  463.134104] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  463.134807] [hdmitx:] set audio
[  463.135290] [hdmitx:] audio_param->chs = 1
[  463.135939] [hdmitx:] aud_src_if = 0
[  463.136528] [hdmitx:] aud_n_para = 5120
[  463.137187] [hdmitx:] audio state: AUDIO_UNMUTE
[  463.137849] [hdmitx:] vinfo: set cur_enc_ppc as 1, vpp color: 0
[  463.138918] DOLBY: vout_notify_callback: VOUT_EVENT_MODE_CHANGE
[  463.139610] vsync_pts_inc 3000 1/30
[  463.140334] [drm] meson_vout_update_mode_name: hdmitx update vout 1 name 2160p30hz.
[  463.157244] [hdmitx:] hdmitx_set_drm_pkt: tf=16, cf=9, colormetry=0
[  463.159643] [snd-soc]: spdif_a is set to disable
[  463.159707] [snd-soc]: aml_audio_reset, reg 0xa, shift 9, use_vadtop 0
[  463.159986] [snd-soc]: aml_audio_reset, reg 0xa, shift 14, use_vadtop 0
[  463.161004] [snd-soc]: hdmitx src switch to spdif 0
[  463.161694] [snd-soc]: sharebuffer_spdifout_prepare  get_hdmitx_audio_src(rtd->card):0  spdif_id:0
[  463.162962] [hdmitx:] hdmitx_audio_notify_callback[798] audio prepare
[  463.163891] [snd-soc]: spdif_a fifo ctrl, frddr:0 type:1, 16 bits, chmask 0x3, swap 0x10
[  463.163901] [hdmitx:] hdmitx_audio_notify_callback[803] type:1 rate:3 size:1 chs:2 i2s_ch_mask:1 aud_src_if:0
[  463.165277] [hdmitx:] aout notify format CT_PCM
[  463.165971] [hdmitx:] set audio
[  463.166508] [hdmitx:] audio_param->chs = 1
[  463.167153] [hdmitx:] aud_src_if = 0
[  463.167741] [hdmitx:] aud_n_para = 5120
[  463.168378] [hdmitx:] audio state: AUDIO_UNMUTE
[  463.169078] [hdmitx:] set audio param
[  463.169743] [snd-soc]: spdif_a is set to enable
[  463.181353] [hdmitx:] avmute_store -1
[  465.384711] [SP FRAME TX] arp req,vif_idx:0 sender:[c0:e3:50:49:af:ae 192.168.0.108]receiver:[00:00:00:00:00:00 192.168.0.106]
[  465.484513] [SP FRAME RX] arp rsp,vif_idx:0 sender:[1c:70:c9:d7:7a:54 192.168.0.106]receiver:[c0:e3:50:49:af:ae 192.168.0.108]
[  467.233344] [hdmitx:] avmute_store 1
[  467.333641] [hdmitx:] phy_store 0
[  467.490928] [drm] [meson_encoder_vrr_change], seamless is 0
[  467.491106] [drm] build_hdmitx_attr_str:422,12bit = 1+12
[  467.492002] [drm] [meson_hdmitx_encoder_atomic_disable]
[  467.492731] [drm] am_meson_crtc_atomic_disable-[0]:in
[  467.493652] [hdmitx:] hdmitx_set_drm_pkt: disable drm pkt
[  467.494379] [hdmitx:] TV not support DV, clr dv_vsif
[  467.495080] [hdmitx:] DV H14b VSIF, switching signal to SDR
[  467.495961] [hdmitx:] hdmitx_set_hdr10plus_pkt: null vsif
[  467.496797] [hdmitx:] hdmitx_unregister_vrr ret = 0
[  467.497439] [drm] am_meson_crtc_atomic_enable-[0] in: new[2160p25hz], old[2160p30hz], vmode[4-4], uboot[0]
[  467.498799] [drm] am_meson_crtc_atomic_enable-[0]: enable mode 2160p25hz final vmode 0
[  467.500200] [hdmitx:] set21_s7d_htxpll_clk_out[96] htxpll vco 5940000 div 2
[  467.501273] [hdmitx:] pll_od0 = 1, pll_od2 = 1, pll_od1 = 2
[  467.501743] [hdmitx:] clocks_set_vid_clk_div_for_hdmi[402] div = 6
[  467.502684] [hdmitx:] configure venc
[  467.503232] [hdmitx:] config_tv_enc_calc[63] vic = 94
[  467.504029] [hdmitx:] hdmitx_soft_reset[1263]
[  467.504708] [hdmitx:]  config hdmitx IP vic = 94 cd:6 cs: 1
[  467.505517] [hdmitx:] configure hdmitx21
[  467.506145] [hdmitx:] warn: SCDC not present, should not send 1:10
[  467.508140] [hdmitx:] enable phy to dig
[  467.508204] [hdmitx:] hdmitx_set_dispmode[1551] frl_rate 0 htotal 5280 cs 1 cd 6 h_unstable 0
[  467.508285] [hdmitx:] hdmitx_set_drm_pkt: tf=1, cf=1, colormetry=0
[  467.510211] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  467.548635] [hdmitx:] set21_phy_by_mode_s7d[188] rterm = 7
[  467.549974] [hdmitx:] Sink is HDMI device
[  467.550136] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  467.550823] [hdmitx:] set audio
[  467.551285] [hdmitx:] audio_param->chs = 1
[  467.551934] [hdmitx:] aud_src_if = 0
[  467.552523] [hdmitx:] aud_n_para = 5120
[  467.553197] [hdmitx:] audio state: AUDIO_UNMUTE
[  467.553847] [hdmitx:] vinfo: set cur_enc_ppc as 1, vpp color: 0
[  467.554917] DOLBY: vout_notify_callback: VOUT_EVENT_MODE_CHANGE
[  467.555602] vsync_pts_inc 3600 1/25
[  467.556324] [drm] meson_vout_update_mode_name: hdmitx update vout 1 name 2160p25hz.
[  467.564476] [snd-soc]: spdif_a is set to disable
[  467.564547] [snd-soc]: aml_audio_reset, reg 0xa, shift 9, use_vadtop 0
[  467.564842] [snd-soc]: aml_audio_reset, reg 0xa, shift 14, use_vadtop 0
[  467.565811] [snd-soc]: hdmitx src switch to spdif 0
[  467.566530] [snd-soc]: sharebuffer_spdifout_prepare  get_hdmitx_audio_src(rtd->card):0  spdif_id:0
[  467.567803] [hdmitx:] hdmitx_audio_notify_callback[798] audio prepare
[  467.568744] [snd-soc]: spdif_a fifo ctrl, frddr:0 type:1, 16 bits, chmask 0x3, swap 0x10
[  467.568755] [hdmitx:] hdmitx_audio_notify_callback[803] type:1 rate:3 size:1 chs:2 i2s_ch_mask:1 aud_src_if:0
[  467.570114] [hdmitx:] aout notify format CT_PCM
[  467.570809] [hdmitx:] set audio
[  467.571348] [hdmitx:] audio_param->chs = 1
[  467.571993] [hdmitx:] aud_src_if = 0
[  467.572599] [hdmitx:] aud_n_para = 5120
[  467.573220] [hdmitx:] audio state: AUDIO_UNMUTE
[  467.573909] [hdmitx:] set audio param
[  467.574592] [snd-soc]: spdif_a is set to enable
[  467.588268] [hdmitx:] hdmitx_set_drm_pkt: tf=16, cf=9, colormetry=0
[  467.612300] [hdmitx:] avmute_store -1
[  471.837880] [hdmitx:] avmute_store 1
[  471.938185] [hdmitx:] phy_store 0
[  472.108553] [drm] build_hdmitx_attr_str:420,8bit = 3+8
[  472.108811] [drm] [meson_hdmitx_encoder_atomic_disable]
[  472.109489] [drm] am_meson_crtc_atomic_disable-[0]:in
[  472.110406] [hdmitx:] hdmitx_set_drm_pkt: disable drm pkt
[  472.111201] [hdmitx:] TV not support DV, clr dv_vsif
[  472.111890] [hdmitx:] DV H14b VSIF, switching signal to SDR
[  472.112821] [hdmitx:] hdmitx_set_hdr10plus_pkt: null vsif
[  472.113602] [hdmitx:] hdmitx_unregister_vrr ret = 0
[  472.114231] [drm] am_meson_crtc_atomic_enable-[0] in: new[2160p50hz], old[2160p25hz], vmode[4-4], uboot[0]
[  472.115596] [drm] am_meson_crtc_atomic_enable-[0]: enable mode 2160p50hz final vmode 0
[  472.117066] [hdmitx:] set21_s7d_htxpll_clk_out[96] htxpll vco 5940000 div 2
[  472.118145] [hdmitx:] pll_od0 = 1, pll_od2 = 0, pll_od1 = 0
[  472.118868] [hdmitx:] clocks_set_vid_clk_div_for_hdmi[402] div = 6
[  472.119472] [hdmitx:] configure venc
[  472.120028] [hdmitx:] config_tv_enc_calc[63] vic = 96
[  472.120864] [hdmitx:] hdmitx_soft_reset[1263]
[  472.121519] [hdmitx:]  config hdmitx IP vic = 96 cd:4 cs: 3
[  472.122365] [hdmitx:] configure hdmitx21
[  472.122947] [hdmitx:] warn: SCDC not present, should not send 1:10
[  472.124911] [hdmitx:] enable phy to dig
[  472.124943] [hdmitx:] hdmitx_set_dispmode[1551] frl_rate 0 htotal 5280 cs 3 cd 4 h_unstable 0
[  472.125026] [hdmitx:] hdmitx_set_drm_pkt: tf=1, cf=1, colormetry=0
[  472.126960] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  472.164635] [hdmitx:] set21_phy_by_mode_s7d[188] rterm = 7
[  472.165970] [hdmitx:] Sink is HDMI device
[  472.166041] [hdmitx:] clear vsif for non-4k mode.
[  472.166691] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  472.167556] [hdmitx:] set audio
[  472.168018] [hdmitx:] audio_param->chs = 1
[  472.168687] [hdmitx:] aud_src_if = 0
[  472.169257] [hdmitx:] aud_n_para = 5120
[  472.169903] [hdmitx:] audio state: AUDIO_UNMUTE
[  472.170575] [hdmitx:] vinfo: set cur_enc_ppc as 1, vpp color: 0
[  472.171738] DOLBY: vout_notify_callback: VOUT_EVENT_MODE_CHANGE
[  472.172337] vsync_pts_inc 1800 1/50
[  472.173160] [drm] meson_vout_update_mode_name: hdmitx update vout 1 name 2160p50hz.
[  472.194494] [snd-soc]: spdif_a is set to disable
[  472.194558] [snd-soc]: aml_audio_reset, reg 0xa, shift 9, use_vadtop 0
[  472.194835] [snd-soc]: aml_audio_reset, reg 0xa, shift 14, use_vadtop 0
[  472.195825] [snd-soc]: hdmitx src switch to spdif 0
[  472.196542] [snd-soc]: sharebuffer_spdifout_prepare  get_hdmitx_audio_src(rtd->card):0  spdif_id:0
[  472.197849] [hdmitx:] hdmitx_audio_notify_callback[798] audio prepare
[  472.198744] [snd-soc]: spdif_a fifo ctrl, frddr:0 type:1, 16 bits, chmask 0x3, swap 0x10
[  472.198758] [hdmitx:] hdmitx_audio_notify_callback[803] type:1 rate:3 size:1 chs:2 i2s_ch_mask:1 aud_src_if:0
[  472.200117] [hdmitx:] aout notify format CT_PCM
[  472.200840] [hdmitx:] set audio
[  472.201361] [hdmitx:] audio_param->chs = 1
[  472.202004] [hdmitx:] aud_src_if = 0
[  472.202614] [hdmitx:] aud_n_para = 5120
[  472.203237] [hdmitx:] audio state: AUDIO_UNMUTE
[  472.203928] [hdmitx:] set audio param
[  472.204668] [snd-soc]: spdif_a is set to enable
[  472.211620] [hdmitx:] avmute_store -1
[  475.914792] [hdmitx:] avmute_store 1
[  476.015116] [hdmitx:] phy_store 0
[  476.145317] [drm] build_hdmitx_attr_str:422,12bit = 1+12
[  476.145569] [drm] [meson_hdmitx_encoder_atomic_disable]
[  476.146246] [drm] am_meson_crtc_atomic_disable-[0]:in
[  476.147156] [hdmitx:] hdmitx_set_drm_pkt: disable drm pkt
[  476.147894] [hdmitx:] TV not support DV, clr dv_vsif
[  476.148644] [hdmitx:] DV H14b VSIF, switching signal to SDR
[  476.149574] [hdmitx:] hdmitx_set_hdr10plus_pkt: null vsif
[  476.150356] [hdmitx:] hdmitx_unregister_vrr ret = 0
[  476.151001] [drm] am_meson_crtc_atomic_enable-[0] in: new[2160p25hz], old[2160p50hz], vmode[4-4], uboot[0]
[  476.152346] [drm] am_meson_crtc_atomic_enable-[0]: enable mode 2160p25hz final vmode 0
[  476.153776] [hdmitx:] set21_s7d_htxpll_clk_out[96] htxpll vco 5940000 div 2
[  476.154803] [hdmitx:] pll_od0 = 1, pll_od2 = 1, pll_od1 = 2
[  476.155292] [hdmitx:] clocks_set_vid_clk_div_for_hdmi[402] div = 6
[  476.156223] [hdmitx:] configure venc
[  476.156808] [hdmitx:] config_tv_enc_calc[63] vic = 94
[  476.157566] [hdmitx:] hdmitx_soft_reset[1263]
[  476.158247] [hdmitx:]  config hdmitx IP vic = 94 cd:6 cs: 1
[  476.159066] [hdmitx:] configure hdmitx21
[  476.159696] [hdmitx:] warn: SCDC not present, should not send 1:10
[  476.161711] [hdmitx:] enable phy to dig
[  476.161756] [hdmitx:] hdmitx_set_dispmode[1551] frl_rate 0 htotal 5280 cs 1 cd 6 h_unstable 0
[  476.204633] [hdmitx:] set21_phy_by_mode_s7d[188] rterm = 7
[  476.205995] [hdmitx:] Sink is HDMI device
[  476.206179] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  476.206878] [hdmitx:] set audio
[  476.207321] [hdmitx:] audio_param->chs = 1
[  476.207969] [hdmitx:] aud_src_if = 0
[  476.208559] [hdmitx:] aud_n_para = 5120
[  476.209241] [hdmitx:] audio state: AUDIO_UNMUTE
[  476.209878] [hdmitx:] vinfo: set cur_enc_ppc as 1, vpp color: 0
[  476.211013] DOLBY: vout_notify_callback: VOUT_EVENT_MODE_CHANGE
[  476.211639] vsync_pts_inc 3600 1/25
[  476.212418] [drm] meson_vout_update_mode_name: hdmitx update vout 1 name 2160p25hz.
[  476.217132] [snd-soc]: spdif_a is set to disable
[  476.217216] [snd-soc]: aml_audio_reset, reg 0xa, shift 9, use_vadtop 0
[  476.217498] [snd-soc]: aml_audio_reset, reg 0xa, shift 14, use_vadtop 0
[  476.218575] [snd-soc]: hdmitx src switch to spdif 0
[  476.219210] [snd-soc]: sharebuffer_spdifout_prepare  get_hdmitx_audio_src(rtd->card):0  spdif_id:0
[  476.220483] [hdmitx:] hdmitx_audio_notify_callback[798] audio prepare
[  476.221452] [snd-soc]: spdif_a fifo ctrl, frddr:0 type:1, 16 bits, chmask 0x3, swap 0x10
[  476.221469] [hdmitx:] hdmitx_audio_notify_callback[803] type:1 rate:3 size:1 chs:2 i2s_ch_mask:1 aud_src_if:0
[  476.222781] [hdmitx:] aout notify format CT_PCM
[  476.223484] [hdmitx:] set audio
[  476.224025] [hdmitx:] audio_param->chs = 1
[  476.224694] [hdmitx:] aud_src_if = 0
[  476.225258] [hdmitx:] aud_n_para = 5120
[  476.225905] [hdmitx:] audio state: AUDIO_UNMUTE
[  476.226586] [hdmitx:] set audio param
[  476.227277] [snd-soc]: spdif_a is set to enable
[  476.241881] [hdmitx:] hdmitx_set_drm_pkt: tf=16, cf=9, colormetry=0
[  476.268093] [hdmitx:] avmute_store -1
[  481.529660] [hdmitx:] avmute_store 1
[  481.629973] [hdmitx:] phy_store 0
[  481.802173] [drm] [meson_encoder_vrr_change], seamless is 0
[  481.802345] [drm] build_hdmitx_attr_str:422,12bit = 1+12
[  481.803233] [drm] [meson_hdmitx_encoder_atomic_disable]
[  481.803934] [drm] am_meson_crtc_atomic_disable-[0]:in
[  481.804839] [hdmitx:] hdmitx_set_drm_pkt: disable drm pkt
[  481.805792] [hdmitx:] TV not support DV, clr dv_vsif
[  481.806342] [hdmitx:] DV H14b VSIF, switching signal to SDR
[  481.807231] [hdmitx:] hdmitx_set_hdr10plus_pkt: null vsif
[  481.808045] [hdmitx:] hdmitx_unregister_vrr ret = 0
[  481.808713] [drm] am_meson_crtc_atomic_enable-[0] in: new[2160p30hz], old[2160p25hz], vmode[4-4], uboot[0]
[  481.810058] [drm] am_meson_crtc_atomic_enable-[0]: enable mode 2160p30hz final vmode 0
[  481.811496] [hdmitx:] set21_s7d_htxpll_clk_out[96] htxpll vco 5940000 div 2
[  481.812556] [hdmitx:] pll_od0 = 1, pll_od2 = 1, pll_od1 = 2
[  481.812984] [hdmitx:] clocks_set_vid_clk_div_for_hdmi[402] div = 6
[  481.813919] [hdmitx:] configure venc
[  481.814474] [hdmitx:] config_tv_enc_calc[63] vic = 95
[  481.815255] [hdmitx:] hdmitx_soft_reset[1263]
[  481.815942] [hdmitx:]  config hdmitx IP vic = 95 cd:6 cs: 1
[  481.817095] [hdmitx:] configure hdmitx21
[  481.817393] [hdmitx:] warn: SCDC not present, should not send 1:10
[  481.819371] [hdmitx:] enable phy to dig
[  481.819417] [hdmitx:] hdmitx_set_dispmode[1551] frl_rate 0 htotal 4400 cs 1 cd 6 h_unstable 0
[  481.819496] [hdmitx:] hdmitx_set_drm_pkt: tf=1, cf=1, colormetry=0
[  481.821430] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  481.856639] [hdmitx:] set21_phy_by_mode_s7d[188] rterm = 7
[  481.857974] [hdmitx:] Sink is HDMI device
[  481.858128] [hdmitx:] hdmitx_set_drm_pkt: hdr.sdr pkt sent
[  481.858822] [hdmitx:] set audio
[  481.859290] [hdmitx:] audio_param->chs = 1
[  481.859958] [hdmitx:] aud_src_if = 0
[  481.860528] [hdmitx:] aud_n_para = 5120
[  481.861221] [hdmitx:] audio state: AUDIO_UNMUTE
[  481.861850] [hdmitx:] vinfo: set cur_enc_ppc as 1, vpp color: 0
[  481.862950] DOLBY: vout_notify_callback: VOUT_EVENT_MODE_CHANGE
[  481.863608] vsync_pts_inc 3000 1/30
[  481.864343] [drm] meson_vout_update_mode_name: hdmitx update vout 1 name 2160p30hz.
[  481.870707] [snd-soc]: spdif_a is set to disable
[  481.870767] [snd-soc]: aml_audio_reset, reg 0xa, shift 9, use_vadtop 0
[  481.871040] [snd-soc]: aml_audio_reset, reg 0xa, shift 14, use_vadtop 0
[  481.872027] [snd-soc]: hdmitx src switch to spdif 0
[  481.872864] [snd-soc]: sharebuffer_spdifout_prepare  get_hdmitx_audio_src(rtd->card):0  spdif_id:0
[  481.874025] [hdmitx:] hdmitx_audio_notify_callback[798] audio prepare
[  481.874951] [snd-soc]: spdif_a fifo ctrl, frddr:0 type:1, 16 bits, chmask 0x3, swap 0x10
[  481.874965] [hdmitx:] hdmitx_audio_notify_callback[803] type:1 rate:3 size:1 chs:2 i2s_ch_mask:1 aud_src_if:0
[  481.876323] [hdmitx:] aout notify format CT_PCM
[  481.877057] [hdmitx:] set audio
[  481.877567] [hdmitx:] audio_param->chs = 1
[  481.878211] [hdmitx:] aud_src_if = 0
[  481.878800] [hdmitx:] aud_n_para = 5120
[  481.879447] [hdmitx:] audio state: AUDIO_UNMUTE
[  481.880135] [hdmitx:] set audio param
[  481.880859] [snd-soc]: spdif_a is set to enable
[  481.886176] [hdmitx:] hdmitx_set_drm_pkt: tf=16, cf=9, colormetry=0
[  481.911074] [hdmitx:] avmute_store -1
[  489.924715] audit: audit_lost=293 audit_rate_limit=5 audit_backlog_limit=64
[  489.924799] type=1400 audit(1753189807.143:1243): avc:  denied  { getattr } for  comm="pkill" path="/proc/1" dev="proc" ino=887 scontext=u:r:su:s0 tcontext=u:r:init:s0 tclass=dir permissive=1
[  489.925048] audit: rate limit exceeded
[  489.928051] type=1400 audit(1753189807.143:1244): avc:  denied  { search } for  comm="pkill" name="1" dev="proc" ino=887 scontext=u:r:su:s0 tcontext=u:r:init:s0 tclass=dir permissive=1
[  489.930289] type=1400 audit(1753189807.143:1245): avc:  denied  { read } for  comm="pkill" name="stat" dev="proc" ino=28571 scontext=u:r:su:s0 tcontext=u:r:init:s0 tclass=file permissive=1
[  489.932415] type=1400 audit(1753189807.143:1246): avc:  denied  { open } for  comm="pkill" path="/proc/1/stat" dev="proc" ino=28571 scontext=u:r:su:s0 tcontext=u:r:init:s0 tclass=file permissive=1
[  489.934759] type=1400 audit(1753189807.147:1247): avc:  denied  { getattr } for  comm="pkill" path="/proc/2" dev="proc" ino=28239 scontext=u:r:su:s0 tcontext=u:r:kernel:s0 tclass=dir permissive=1
[  508.904745] [aml_send_sync_trace 4388] sync token[36946]
[  508.904768] >>> aml_send_msg()
[  508.905698] ipc_sdio_host_msgack_handler 000000001348513f
[  508.906222] [aml_msgackind 2039] msg ack hostid=0xffffff80718e1a00
[  508.907131] [cmd_mgr_llind         329] cmd tkn[45]  flags:0008  result: -4  cmd: 105-MM_SYNC_TRACE            - reqcfm(   0-none)
[  508.908780] [cmd_complete           65] cmd tkn[45]  flags:0000  result: -4  cmd: 105-MM_SYNC_TRACE            - reqcfm(   0-none)
[  516.328679] [SP FRAME TX] arp req,vif_idx:0 sender:[c0:e3:50:49:af:ae 192.168.0.108]receiver:[00:00:00:00:00:00 192.168.0.1]
[  516.331620] [SP FRAME RX] arp rsp,vif_idx:0 sender:[f8:8c:21:8f:40:25 192.168.0.1]receiver:[c0:e3:50:49:af:ae 192.168.0.108]
[  517.569987] type=1400 audit(1753189834.791:1577): avc:  denied  { search } for  comm="cat" name="amhdmitx0" dev="sysfs" ino=30902 scontext=u:r:su:s0 tcontext=u:object_r:sysfs_amhdmitx:s0 tclass=dir permissive=1
[  517.571950] type=1400 audit(1753189834.791:1578): avc:  denied  { read } for  comm="cat" name="rawedid" dev="sysfs" ino=31189 scontext=u:r:su:s0 tcontext=u:object_r:sysfs_amhdmitx:s0 tclass=file permissive=1
[  517.574616] type=1400 audit(1753189834.791:1579): avc:  denied  { open } for  comm="cat" path="/sys/devices/virtual/amhdmitx/amhdmitx0/rawedid" dev="sysfs" ino=31189 scontext=u:r:su:s0 tcontext=u:object_r:sysfs_amhdmitx:s0 tclass=file permissive=1
[  545.256665] [SP FRAME TX] arp req,vif_idx:0 sender:[c0:e3:50:49:af:ae 192.168.0.108]receiver:[00:00:00:00:00:00 192.168.0.106]
[  545.359082] [SP FRAME RX] arp rsp,vif_idx:0 sender:[1c:70:c9:d7:7a:54 192.168.0.106]receiver:[c0:e3:50:49:af:ae 192.168.0.108]
[  565.849320] type=1400 audit(1753189883.071:1580): avc:  denied  { connectto } for  comm=75736220666673206F70656E path="/dev/socket/property_service" scontext=u:r:su:s0 tcontext=u:r:init:s0 tclass=unix_stream_socket permissive=1
[  570.344629] [aml_send_sync_trace 4388] sync token[36947]
[  570.344653] >>> aml_send_msg()
[  570.345567] ipc_sdio_host_msgack_handler 000000002bbd2fa7
[  570.346109] [aml_msgackind 2039] msg ack hostid=0xffffff807e7d2700
[  570.347017] [cmd_mgr_llind         329] cmd tkn[46]  flags:0008  result: -4  cmd: 105-MM_SYNC_TRACE            - reqcfm(   0-none)
[  570.348646] [cmd_complete           65] cmd tkn[46]  flags:0000  result: -4  cmd: 105-MM_SYNC_TRACE            - reqcfm(   0-none)
[  572.136679] [SP FRAME TX] arp req,vif_idx:0 sender:[c0:e3:50:49:af:ae 192.168.0.108]receiver:[00:00:00:00:00:00 192.168.0.106]
[  572.141884] [SP FRAME RX] arp rsp,vif_idx:0 sender:[1c:70:c9:d7:7a:54 192.168.0.106]receiver:[c0:e3:50:49:af:ae 192.168.0.108]
[  598.248675] [SP FRAME TX] arp req,vif_idx:0 sender:[c0:e3:50:49:af:ae 192.168.0.108]receiver:[00:00:00:00:00:00 192.168.0.106]
[  598.322253] [SP FRAME RX] arp rsp,vif_idx:0 sender:[1c:70:c9:d7:7a:54 192.168.0.106]receiver:[c0:e3:50:49:af:ae 192.168.0.108]
[  606.134599] type=1400 audit(1753189923.355:1581): avc:  denied  { search } for  comm="sh" name="/" dev="fuse" ino=131 scontext=u:r:su:s0 tcontext=u:object_r:fuse:s0 tclass=dir permissive=1
[  606.164020] type=1400 audit(1753189923.383:1582): avc:  denied  { ioctl } for  comm="dmesg" path="/storage/emulated/0/dmesg.txt" dev="fuse" ino=5186 ioctlcmd=0x5401 scontext=u:r:su:s0 tcontext=u:object_r:fuse:s0 tclass=file permissive=1
[  606.166253] type=1400 audit(1753189923.383:1583): avc:  denied  { read } for  comm="dmesg" name="kmsg" dev="tmpfs" ino=5 scontext=u:r:su:s0 tcontext=u:object_r:kmsg_device:s0 tclass=chr_file permissive=1
[  606.168597] type=1400 audit(1753189923.383:1584): avc:  denied  { open } for  comm="dmesg" path="/dev/kmsg" dev="tmpfs" ino=5 scontext=u:r:su:s0 tcontext=u:object_r:kmsg_device:s0 tclass=chr_file permissive=1
[  606.171025] type=1400 audit(1753189923.383:1585): avc:  denied  { syslog_read } for  comm="dmesg" scontext=u:r:su:s0 tcontext=u:r:kernel:s0 tclass=system permissive=1
